<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;b&gt;Linear Technology Devices&lt;/b&gt;&lt;p&gt;
http://www.linear-tech.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="Q5-DD">
<description>&lt;b&gt;Q5-DD&lt;/b&gt;</description>
</package>
<package name="TO220-5">
<description>&lt;b&gt;TO220-5&lt;/b&gt;</description>
</package>
<package name="DDPACK-5">
<description>DDPACK-5</description>
</package>
<package name="DDPACK-7+TAB">
<description>DDPACK 7</description>
</package>
<package name="TO220-7">
</package>
<package name="MS10">
</package>
<package name="MS10-THERM">
</package>
<package name="DFN10">
<description>DFN-10 (3mmx3mm)</description>
</package>
<package name="TSSOP16-BC">
<description>&lt;b&gt;TSSOP16-BC&lt;/b&gt; - FE Package&lt;p&gt;
Exposed pad variation BC</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="MSOP08">
<description>&lt;b&gt;Mini Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP-36W">
</package>
<package name="SSOP16-5">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt; - 5.3 mm body variant</description>
</package>
<package name="TO263-5">
<description>&lt;b&gt;TO-263&lt;/b&gt;</description>
</package>
<package name="TO263-7">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="SO14">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
<package name="SO16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="DFN12-3X3">
<description>DFN 3x3mm, 12 lead</description>
</package>
<package name="MSOP12-MSE">
<description>MSOP12-MSE</description>
</package>
<package name="QFN52-UKG">
<description>&lt;b&gt;52-Lead Plastic QFN&lt;/b&gt;&lt;p&gt;
body 7mm × 8mm, UKG Package</description>
</package>
<package name="TSOT23-6">
<description>&lt;b&gt;TSOT-23&lt;/b&gt; - S6&lt;p&gt;
0.95 mm pitch</description>
</package>
<package name="DFN6-2X3">
<description>DCB Package&lt;p&gt;
6-Lead Plastic DFN (2mm × 3mm)&lt;p&gt;
(Reference LTC DWG # 05-08-1715 Rev A)</description>
</package>
<package name="DFN8-3X3">
<description>&lt;b&gt;DFN-8&lt;/b&gt;&lt;p&gt;
3x3mm body</description>
</package>
<package name="DFN10-3X3">
<description>DFN-10 (3mmx3mm)</description>
</package>
<package name="LGA50-SMD">
<description>&lt;b&gt;LGA 50 Package&lt;/b&gt;&lt;p&gt;
11.25mm × 9.00mm × 2.82mm&lt;p&gt;
Solder Mask Defined Pads (0.63 mm opening)</description>
</package>
<package name="QFN40-UJ">
<description>&lt;b&gt;QFN-40 UJ Package&lt;/b&gt;&lt;p&gt;
40-Lead (6mm × 6mm) Plastic QFN&lt;p&gt;
(Reference LTC DWG # 05-08-1728)</description>
</package>
<package name="QFN16-UD">
<description>&lt;b&gt;QFN16&lt;/b&gt;&lt;p&gt;
body 3 x 3 x 0.75 mm</description>
</package>
<package name="MSOP16-MSE">
<description>MSOP16-MSE</description>
</package>
<package name="SC70-6W">
<description>&lt;b&gt;SC70&lt;/b&gt;&lt;p&gt;
0.65 mm pitch</description>
</package>
<package name="QFN10-UDB">
<description>10-Lead Plastic QFN&lt;p&gt;
body  3 × 2 mm</description>
</package>
<package name="DFN8-DDB">
<description>&lt;b&gt;DFN8 - DDB Package&lt;/b&gt;&lt;p&gt;
8-Lead Plastic DFN (3mm × 2mm)</description>
</package>
<package name="QFN20-UDC">
<description>&lt;b&gt;QFN20 - UDC&lt;/b&gt;&lt;p&gt;
body 3 x 4 mm</description>
</package>
<package name="BLGA32">
<description>&lt;b&gt;BLGA Package&lt;/b&gt;&lt;p&gt;
32-Lead (15mm × 11.25mm × 2.82mm)&lt;p&gt;
Pitch 0.635mm
(Reference LTC DWG # 05-08-1773 Rev Ø)</description>
</package>
<package name="SOT23-8">
<description>&lt;b&gt;SOT-23&lt;/b&gt; - DCN&lt;p&gt;
0.65 mm pitch</description>
</package>
<package name="DFN8-DC">
<description>8-Lead Plastic DFN (2mm × 2mm)&lt;p&gt;
DC Package&lt;p&gt;
(Reference LTC DWG # 05-08-1719 Rev Ø)</description>
</package>
<package name="MSOP16-MS16(12)">
<description>MSOP16-MS16(12)&lt;p&gt;
Varitation: MS16 (12)&lt;p&gt;
16-Lead Plastic MSOP with 4 Pins Removed</description>
</package>
<package name="TSSOP20-CB">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
FE Package 20-Lead Plastic TSSOP (4.4mm)&lt;p&gt;
(Reference LTC DWG # 05-08-1663 Rev J)&lt;br&gt;
Exposed Pad Variation CB</description>
</package>
<package name="TSOT23-8">
<description>&lt;b&gt;TSOT-23&lt;/b&gt; - TS8&lt;p&gt;
0.65 mm pitch</description>
</package>
<package name="DFN18">
<description>&lt;b&gt;DFN-18&lt;/b&gt; - DHC Package&lt;p&gt;
18-Lead Plastic DFN (5mm × 3mm)</description>
</package>
<package name="BGA25">
<description>&lt;b&gt;BGA25&lt;/b&gt;&lt;p&gt;
25-Lead (6.25mm × 6.25mm × 2.42mm)&lt;p&gt;
Reference LTC DWG # 05-08-1502</description>
</package>
<package name="QFN-64">
</package>
</packages>
<symbols>
<symbol name="LT1129">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!SHDN!" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="LT1129-3">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1016">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="LA_EN" direction="in"/>
<pin name="!OUT" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LTC1658">
<pin name="DOUT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="!CSLD" direction="in"/>
</symbol>
<symbol name="LTC1440">
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="HYST" direction="pas"/>
<pin name="REF" direction="out"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWRN">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1764A">
<pin name="IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
<pin name="!SHDN!" direction="in"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="TAB" direction="pwr"/>
</symbol>
<symbol name="LT1716">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LT1512">
<pin name="VIN" direction="pwr"/>
<pin name="VSW" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="IFB" direction="pas"/>
<pin name="GND1@2" direction="pwr"/>
<pin name="VC" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="S/S" direction="pas"/>
</symbol>
<symbol name="LT1370T">
<pin name="FB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VSW" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="S/S" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="NFB" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="LT1370">
<pin name="FB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VSW" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="S/S" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="NFB" direction="in"/>
</symbol>
<symbol name="LT1025">
<pin name="VIN" direction="pwr"/>
<pin name="K" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="R-" direction="pas"/>
</symbol>
<symbol name="LTC1261L">
<pin name="REG" direction="out"/>
<pin name="SHDN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="ADJ" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LT1637">
<pin name="NULL1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="NULL2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="SHDN" direction="pas"/>
</symbol>
<symbol name="LT1269">
<pin name="FB" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VSW" direction="pas"/>
<pin name="VIN" direction="pwr"/>
<pin name="VC" direction="pas"/>
</symbol>
<symbol name="LT1910">
<pin name="IN" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="!FAULT!" direction="out"/>
<pin name="SENSE" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="TIMER" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LT107X">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="VC"/>
<pin name="VSW"/>
<pin name="FB"/>
</symbol>
<symbol name="ITC137P">
<pin name="C" direction="pwr"/>
<pin name="B" direction="pwr"/>
<pin name="E" direction="pwr"/>
<pin name="BRG" direction="pwr"/>
<pin name="Z2"/>
<pin name="Z3"/>
<pin name="Z1"/>
<pin name="TIP"/>
<pin name="T"/>
<pin name="RDET"/>
<pin name="RING"/>
<pin name="OH-"/>
<pin name="OH+"/>
<pin name="RI-"/>
<pin name="RI+"/>
</symbol>
<symbol name="LT117X">
<pin name="VSW" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="VC" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="E"/>
</symbol>
<symbol name="LT1370CR">
<pin name="VIN"/>
<pin name="S/S"/>
<pin name="GND"/>
<pin name="NFB"/>
<pin name="VSW"/>
<pin name="FB"/>
<pin name="VC"/>
</symbol>
<symbol name="LT1374">
<pin name="VIN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="BOOST"/>
<pin name="VSW"/>
<pin name="SENSE"/>
<pin name="VC"/>
</symbol>
<symbol name="LT1513">
<pin name="VIN"/>
<pin name="S/S"/>
<pin name="VC"/>
<pin name="GND"/>
<pin name="IFB"/>
<pin name="VSW"/>
<pin name="VFB"/>
</symbol>
<symbol name="LT1615">
<pin name="VIN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="LT1761-BYP">
<pin name="IN"/>
<pin name="BYP"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="ADJ"/>
</symbol>
<symbol name="LTC1155">
<pin name="DS1"/>
<pin name="G1"/>
<pin name="GND"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="VS"/>
<pin name="G2"/>
<pin name="DS2"/>
</symbol>
<symbol name="LTC1732">
<pin name="!CHRG!"/>
<pin name="!ACPR!"/>
<pin name="PROG"/>
<pin name="TIMER"/>
<pin name="GND"/>
<pin name="BAT"/>
<pin name="DRV"/>
<pin name="SENSE"/>
<pin name="SEL"/>
<pin name="VCC"/>
</symbol>
<symbol name="LT1735">
<pin name="COSC"/>
<pin name="RUN/SS"/>
<pin name="ITH"/>
<pin name="FCB"/>
<pin name="SGND"/>
<pin name="SENSE-"/>
<pin name="SENSE+"/>
<pin name="VOSENSE"/>
<pin name="EXTVCC"/>
<pin name="PGND"/>
<pin name="BG"/>
<pin name="INTVCC"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="BOOST"/>
<pin name="TG"/>
</symbol>
<symbol name="LTC1877">
<pin name="SYNC"/>
<pin name="VIN"/>
<pin name="RUN"/>
<pin name="ITH"/>
<pin name="GND" direction="pwr"/>
<pin name="VFB"/>
<pin name="SW"/>
<pin name="PLL"/>
</symbol>
<symbol name="LTC3407">
<pin name="VIN"/>
<pin name="MODE/SYNC"/>
<pin name="RUN1"/>
<pin name="RUN2"/>
<pin name="!POR!"/>
<pin name="GND"/>
<pin name="SW1"/>
<pin name="VFB1"/>
<pin name="SW2"/>
<pin name="VFB2"/>
<pin name="HS"/>
</symbol>
<symbol name="LT3800">
<pin name="VIN" direction="in"/>
<pin name="BURST_EN"/>
<pin name="!SHDN!" direction="in"/>
<pin name="CSS"/>
<pin name="VFB"/>
<pin name="VC"/>
<pin name="SENSE-" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="SGND" direction="pwr"/>
<pin name="NC2" direction="nc"/>
<pin name="SENSE+" direction="in"/>
<pin name="PGND"/>
<pin name="BG" direction="out"/>
<pin name="VCC"/>
<pin name="SW"/>
<pin name="TG"/>
<pin name="BOOST"/>
</symbol>
<symbol name="LT1620IS8">
<pin name="IN-" direction="in"/>
<pin name="SENSE" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="PROG"/>
<pin name="AVG"/>
</symbol>
<symbol name="LT2606">
<pin name="SCL"/>
<pin name="VCC" direction="pwr"/>
<pin name="!LDAC!" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="SDA"/>
<pin name="CA0"/>
<pin name="CA1"/>
<pin name="CA2"/>
</symbol>
<symbol name="LT1676">
<pin name="FB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VSW" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="SYNC" direction="in"/>
</symbol>
<symbol name="LTC3406">
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SW" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="RUN" direction="in"/>
</symbol>
<symbol name="LT3471">
<pin name="VIN"/>
<pin name="!SHDN1!"/>
<pin name="!SHDN2!"/>
<pin name="VREF"/>
<pin name="GND"/>
<pin name="SW1"/>
<pin name="FB1N"/>
<pin name="SW2"/>
<pin name="FB2N"/>
<pin name="FB1P"/>
<pin name="FB2P"/>
</symbol>
<symbol name="LT1761-SD">
<pin name="IN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="ADJ"/>
</symbol>
<symbol name="LT1761">
<pin name="IN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="BYP"/>
</symbol>
<symbol name="LT1964">
<pin name="IN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="BYP"/>
</symbol>
<symbol name="LT1964-BYP">
<pin name="IN"/>
<pin name="BYP"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="ADJ"/>
</symbol>
<symbol name="LT1964-SD">
<pin name="IN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="ADJ"/>
</symbol>
<symbol name="LT1791">
<pin name="Z" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="RO" direction="out"/>
<pin name="DE" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="!RE!" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LTC1564">
<pin name="AGND" direction="pwr"/>
<pin name="!EN!" direction="in"/>
<pin name="F0" direction="in"/>
<pin name="F1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="F3" direction="in"/>
<pin name="G0" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="G2" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="in"/>
<pin name="!RST!" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LTC1821">
<pin name="AGNDF" direction="pwr"/>
<pin name="AGNDS" direction="pwr"/>
<pin name="!CLR!" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D15" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="DNC@1" direction="nc"/>
<pin name="DNC@2" direction="nc"/>
<pin name="DNC@3" direction="nc"/>
<pin name="IOUT" direction="out"/>
<pin name="!LD!" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="R1" direction="in"/>
<pin name="RCOM" direction="out"/>
<pin name="REF" direction="in"/>
<pin name="RFB" direction="out"/>
<pin name="ROFS" direction="in"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="VCC"/>
<pin name="VOUT" direction="out"/>
<pin name="!WR!" direction="in"/>
</symbol>
<symbol name="LT1460">
<pin name="GND" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LTC1966">
<pin name="OUT-RTN" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IN2" direction="in"/>
<pin name="!EN!" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LTC6905">
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="OUT"/>
<pin name="DIV" direction="in"/>
</symbol>
<symbol name="LT6650">
<pin name="IN" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="LT3430">
<pin name="VIN@3" direction="in"/>
<pin name="BOOST" direction="pwr"/>
<pin name="BIAS" direction="pas"/>
<pin name="SW@2" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="SW@5" direction="out"/>
<pin name="VIN@4" direction="in"/>
<pin name="!SHDN!" direction="in"/>
<pin name="SYNC" direction="pas"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="FB" direction="pas"/>
<pin name="VC" direction="pas"/>
</symbol>
<symbol name="1963AEQ">
<pin name="IN" direction="in"/>
<pin name="!SHDN!" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="SENSE" direction="pas"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="LT1054">
<pin name="FB/SHDN"/>
<pin name="CAP+"/>
<pin name="GND"/>
<pin name="CAP-"/>
<pin name="VOUT"/>
<pin name="VREF"/>
<pin name="OSC"/>
<pin name="V+"/>
</symbol>
<symbol name="LTC1481">
<pin name="RO"/>
<pin name="!RE"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="VCC"/>
<pin name="B"/>
<pin name="A"/>
<pin name="GND"/>
</symbol>
<symbol name="LT3652">
<pin name="VIN" direction="in"/>
<pin name="VIN_REG" direction="in"/>
<pin name="!SHDN!" direction="in"/>
<pin name="!CHRG!" direction="oc"/>
<pin name="!FAULT!" direction="oc"/>
<pin name="TIMER" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="NTC" direction="in"/>
<pin name="BAT" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="BOOST" direction="in"/>
<pin name="SW" direction="in"/>
</symbol>
<symbol name="LTC4411">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="CTL" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="STAT" direction="out"/>
</symbol>
<symbol name="LTC2173/74/75">
<pin name="AIN1+" direction="in"/>
<pin name="AIN1-" direction="in"/>
<pin name="VCM12" direction="out"/>
<pin name="AIN2+" direction="in"/>
<pin name="AIN2-" direction="in"/>
<pin name="REFH@6" direction="pas"/>
<pin name="REFH@7" direction="pas"/>
<pin name="REFL@8" direction="pas"/>
<pin name="REFL@9" direction="pas"/>
<pin name="AIN3+" direction="in"/>
<pin name="AIN3-" direction="in"/>
<pin name="VCM34" direction="pas"/>
<pin name="AIN4+" direction="in"/>
<pin name="AIN4-" direction="in"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="ENC+" direction="in"/>
<pin name="ENC-" direction="in"/>
<pin name="!CS!" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="GND@22" direction="pwr"/>
<pin name="OUT4B-" direction="out"/>
<pin name="OUT4B+" direction="out"/>
<pin name="OUT4A-" direction="out"/>
<pin name="OUT4A+" direction="out"/>
<pin name="OUT3B-" direction="out"/>
<pin name="OUT3B+" direction="out"/>
<pin name="OUT3A-" direction="out"/>
<pin name="OUT3A+" direction="out"/>
<pin name="FR-" direction="out"/>
<pin name="FR+" direction="out"/>
<pin name="OGND" direction="pwr"/>
<pin name="OVDD" direction="pwr"/>
<pin name="DCO-" direction="out"/>
<pin name="DCO+" direction="out"/>
<pin name="OUT2B-" direction="out"/>
<pin name="OUT2B+" direction="out"/>
<pin name="OUT2A-" direction="out"/>
<pin name="OUT2A+" direction="out"/>
<pin name="OUT1B-" direction="out"/>
<pin name="OUT1B+" direction="out"/>
<pin name="OUT1A-" direction="out"/>
<pin name="OUT1A+" direction="out"/>
<pin name="GND@45" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="PAR/!SER!" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="GND@49" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="VDD@51" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
</symbol>
<symbol name="LTC4412">
<pin name="VIN" direction="in"/>
<pin name="CTL" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="STAT" direction="out"/>
<pin name="GATE" direction="out"/>
<pin name="SENSE" direction="in"/>
</symbol>
<symbol name="LT1763">
<pin name="IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
<pin name="!SHDN!" direction="in"/>
<pin name="SEN" direction="pas"/>
<pin name="GND@3" direction="pwr"/>
<pin name="BYP" direction="pas"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
</symbol>
<symbol name="LTC4357">
<pin name="IN" direction="pwr"/>
<pin name="GATE" direction="out"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pas"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="LTC485">
<pin name="RO" direction="out"/>
<pin name="!RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LTM8022">
<pin name="IN@G1" direction="in"/>
<pin name="RUN/SS" direction="in"/>
<pin name="OUT@A1" direction="pas"/>
<pin name="AUX" direction="pas"/>
<pin name="BIAS" direction="in"/>
<pin name="PG" direction="oc"/>
<pin name="ADJ" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="GND@A5" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="SHARE" direction="pas"/>
<pin name="IN@G2" direction="in"/>
<pin name="IN@G3" direction="in"/>
<pin name="IN@H1" direction="in"/>
<pin name="IN@H2" direction="in"/>
<pin name="IN@H3" direction="in"/>
<pin name="OUT@A2" direction="pas"/>
<pin name="OUT@A3" direction="pas"/>
<pin name="OUT@B1" direction="pas"/>
<pin name="OUT@B2" direction="pas"/>
<pin name="OUT@B3" direction="pas"/>
<pin name="OUT@A4" direction="pas"/>
<pin name="OUT@B4" direction="pas"/>
<pin name="OUT@C1" direction="pas"/>
<pin name="OUT@C2" direction="pas"/>
<pin name="OUT@C3" direction="pas"/>
<pin name="OUT@C4" direction="pas"/>
<pin name="GND@A6" direction="in"/>
<pin name="GND@A7" direction="in"/>
<pin name="GND@B5" direction="in"/>
<pin name="GND@B6" direction="in"/>
<pin name="GND@B7" direction="in"/>
<pin name="GND@C5" direction="in"/>
<pin name="GND@C6" direction="in"/>
<pin name="GND@C7" direction="in"/>
<pin name="GND@D1" direction="in"/>
<pin name="GND@E1" direction="in"/>
<pin name="GND@D2" direction="in"/>
<pin name="GND@D3" direction="in"/>
<pin name="GND@D4" direction="in"/>
<pin name="GND@D5" direction="in"/>
<pin name="GND@D6" direction="in"/>
<pin name="GND@D7" direction="in"/>
<pin name="GND@E2" direction="in"/>
<pin name="GND@E3" direction="in"/>
<pin name="GND@E4" direction="in"/>
<pin name="GND@E5" direction="in"/>
<pin name="GND@E6" direction="in"/>
<pin name="GND@E7" direction="in"/>
<pin name="GND@F6" direction="in"/>
</symbol>
<symbol name="LTC6102">
<pin name="-INS" direction="in"/>
<pin name="-INF" direction="in"/>
<pin name="V-/EN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="VREG" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="+IN" direction="in"/>
</symbol>
<symbol name="LTC4413-2">
<pin name="INA" direction="in"/>
<pin name="ENBA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="ENBB" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="OVP" direction="out"/>
<pin name="OVI" direction="in"/>
<pin name="STAT" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LTC4413-1">
<pin name="INA" direction="in"/>
<pin name="ENBA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="ENBB" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="NC@7" direction="out"/>
<pin name="NC@8" direction="in"/>
<pin name="STAT" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="LTC2266/67/68-14">
<pin name="AIN1+" direction="in"/>
<pin name="AIN1-" direction="in"/>
<pin name="VCM1" direction="out"/>
<pin name="REFH@4" direction="pwr"/>
<pin name="REFH@5" direction="pwr"/>
<pin name="REFL@6" direction="pwr"/>
<pin name="REFL@7" direction="pwr"/>
<pin name="VCM2" direction="out"/>
<pin name="AIN2+" direction="in"/>
<pin name="AIN2-" direction="in"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="ENC+" direction="in"/>
<pin name="ENC-" direction="in"/>
<pin name="!CS!" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="GND@13" direction="pwr"/>
<pin name="OUT2B-" direction="out"/>
<pin name="OUT2B+" direction="out"/>
<pin name="OUT2A-" direction="out"/>
<pin name="OUT2A+" direction="out"/>
<pin name="FR-" direction="out"/>
<pin name="FR+" direction="out"/>
<pin name="OGND" direction="pwr"/>
<pin name="OVDD" direction="pwr"/>
<pin name="DCO-" direction="out"/>
<pin name="DCO+" direction="out"/>
<pin name="OUT1B-" direction="out"/>
<pin name="OUT1B+" direction="out"/>
<pin name="OUT1A-" direction="out"/>
<pin name="OUT1A+" direction="out"/>
<pin name="GND@$33" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="PAR/!SER!" direction="in"/>
<pin name="VREF" direction="hiz"/>
<pin name="GND@37" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
</symbol>
<symbol name="LTC3601UD">
<pin name="MODE/SYNC" direction="in"/>
<pin name="PGOOD" direction="oc"/>
<pin name="SW@3" direction="out"/>
<pin name="SW@4" direction="out"/>
<pin name="NC@5" direction="nc"/>
<pin name="BOOST" direction="in"/>
<pin name="INTVCC" direction="out"/>
<pin name="VON" direction="in"/>
<pin name="SGND" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ITH" direction="in"/>
<pin name="TRACK" direction="in"/>
<pin name="RUN" direction="in"/>
<pin name="VIN@15" direction="pwr"/>
<pin name="VIN@16" direction="pwr"/>
</symbol>
<symbol name="LTC3601MSE">
<pin name="MODE/SYNC" direction="in"/>
<pin name="PGOOD" direction="oc"/>
<pin name="SW@1" direction="out"/>
<pin name="SW@2" direction="out"/>
<pin name="PGND@3" direction="pwr"/>
<pin name="BOOST" direction="in"/>
<pin name="INTVCC" direction="out"/>
<pin name="VON" direction="in"/>
<pin name="PGND@4" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ITH" direction="in"/>
<pin name="TRACK" direction="in"/>
<pin name="RUN" direction="in"/>
<pin name="VIN@13" direction="pwr"/>
<pin name="VIN@14" direction="pwr"/>
</symbol>
<symbol name="LT5534">
<pin name="EN" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="RF" direction="in"/>
</symbol>
<symbol name="LTC6409">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-OUT" direction="out"/>
<pin name="+OUT" direction="out"/>
<pin name="V+@4" direction="pwr"/>
<pin name="V-@8" direction="pwr"/>
<pin name="!SHDN!" direction="in"/>
<pin name="VOCM" direction="in"/>
<pin name="V+@9" direction="pwr"/>
<pin name="V-@10" direction="pwr"/>
<pin name="V-@11" direction="pwr"/>
</symbol>
<symbol name="LT3092">
<pin name="SET" direction="in"/>
<pin name="IN@7" direction="pas"/>
<pin name="OUT@1" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="IN@8" direction="pas"/>
<pin name="OUT@9" direction="pas"/>
</symbol>
<symbol name="LTC1799">
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIV" direction="pas"/>
</symbol>
<symbol name="LTC2954">
<pin name="VIN" direction="pwr"/>
<pin name="PB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="ONT" direction="pas"/>
<pin name="PDT" direction="pas"/>
<pin name="!KILL!" direction="in"/>
<pin name="!INT!" direction="oc"/>
<pin name="!EN!" direction="oc"/>
</symbol>
<symbol name="LTC4099">
<pin name="OVGATE" direction="out"/>
<pin name="NTC" direction="pas"/>
<pin name="NTCBIAS" direction="pas"/>
<pin name="VC" direction="out"/>
<pin name="WALL" direction="in"/>
<pin name="BATSENS" direction="in"/>
<pin name="PROG" direction="pas"/>
<pin name="!IRQ!" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="IDGATE" direction="out"/>
<pin name="BAT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="VBUS" direction="in"/>
<pin name="SW" direction="out"/>
<pin name="DVCC" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="!ACPR!" direction="out"/>
<pin name="CLPROG" direction="pas"/>
<pin name="OVSENS" direction="in"/>
<pin name="GND@21" direction="pwr"/>
</symbol>
<symbol name="LTC2953">
<pin name="GND"/>
<pin name="VM"/>
<pin name="!KILL!"/>
<pin name="PDT"/>
<pin name="!PB!"/>
<pin name="VIN"/>
<pin name="UVLO"/>
<pin name="!PFI!"/>
<pin name="!PFO!"/>
<pin name="EN/!EN!"/>
<pin name="!RST!"/>
<pin name="!INT!"/>
</symbol>
<symbol name="LTC2942-1">
<pin name="!AL!/CC"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SENSE-" direction="in"/>
<pin name="SENSE+" direction="in"/>
</symbol>
<symbol name="LTM2882">
<pin name="R2OUT" direction="out"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="ON" direction="in"/>
<pin name="VL" direction="pwr"/>
<pin name="GND@B1" direction="pwr"/>
<pin name="GBD@B2" direction="pwr"/>
<pin name="GND@B3" direction="pwr"/>
<pin name="GND@B4" direction="pwr"/>
<pin name="GND@B5" direction="pwr"/>
<pin name="GND@B6" direction="pwr"/>
<pin name="VCC@A8" direction="pwr"/>
<pin name="VCC@B8" direction="pwr"/>
<pin name="VCC@B7" direction="pwr"/>
<pin name="GND2@K1" direction="pas"/>
<pin name="GND2@K2" direction="pas"/>
<pin name="GND2@K3" direction="pas"/>
<pin name="GND2@K4" direction="pas"/>
<pin name="GND2@K5" direction="pas"/>
<pin name="GND2@K6" direction="pas"/>
<pin name="VCC2@K8" direction="pas"/>
<pin name="VCC2@L8" direction="pas"/>
<pin name="VCC2@L7" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="T2OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="GND2@K7" direction="pas"/>
</symbol>
<symbol name="LTC2935">
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="!MR!" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="!RST!" direction="out"/>
<pin name="!PFO!" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LT1762-ADJ">
<pin name="IN"/>
<pin name="!SHDN!"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="ADJ"/>
<pin name="BYP"/>
</symbol>
<symbol name="LTC5507">
<pin name="VCC" direction="pwr"/>
<pin name="PCAP" direction="pas"/>
<pin name="RFIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="!SHDN!" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="LT3748">
<pin name="VIN" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="RREF" direction="in"/>
<pin name="EN/UVLO" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="GATE" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="TC" direction="pas"/>
<pin name="SS" direction="pas"/>
<pin name="VC" direction="pas"/>
<pin name="INTVCC" direction="pas"/>
</symbol>
<symbol name="LT3015-ADJ">
<pin name="IN" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LT1963A">
<pin name="IN" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LT3080">
<pin name="IN" direction="in"/>
<pin name="VCTL" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="LT1962">
<pin name="IN" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="BYP" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="SENSE/ADJ" direction="pas"/>
</symbol>
<symbol name="LT8471">
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="SHOUT" direction="out"/>
<pin name="C3" direction="in"/>
<pin name="OV/UV" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="SYNC"/>
<pin name="RT" direction="in"/>
<pin name="PG1" direction="oc"/>
<pin name="PG2" direction="oc"/>
<pin name="E2" direction="out"/>
<pin name="FB2" direction="in"/>
<pin name="C2" direction="oc"/>
<pin name="GND@10" direction="pwr"/>
<pin name="E1" direction="out"/>
<pin name="FB1" direction="in"/>
<pin name="C1" direction="oc"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
</symbol>
<symbol name="LTC4011">
<pin name="DCIN" direction="in"/>
<pin name="!FAULT!" direction="oc"/>
<pin name="!CHRG!" direction="oc"/>
<pin name="CHEM" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VRT" direction="out"/>
<pin name="VTEMP" direction="in"/>
<pin name="VCELL" direction="in"/>
<pin name="VCDIV" direction="oc"/>
<pin name="TIMER" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="BAT" direction="pas"/>
<pin name="!TOC!" direction="oc"/>
<pin name="INTVDD" direction="out"/>
<pin name="BGATE" direction="out"/>
<pin name="PGND" direction="pas"/>
<pin name="TGATE" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="!READY!" direction="out"/>
<pin name="INFET" direction="out"/>
<pin name="EXPAD" direction="pas"/>
</symbol>
<symbol name="LTC4365">
<pin name="VIN" direction="in"/>
<pin name="!SHDN!"/>
<pin name="UV" direction="in"/>
<pin name="0V" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="!FAULT!" direction="oc"/>
<pin name="VOUT" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="LTC3265">
<pin name="CBST-" direction="in"/>
<pin name="CBST+" direction="in"/>
<pin name="VIN_P" direction="in"/>
<pin name="EN-" direction="in"/>
<pin name="BYP-" direction="in"/>
<pin name="ADJ-" direction="in"/>
<pin name="LDO-" direction="in"/>
<pin name="VOUT-" direction="pas"/>
<pin name="CINV-" direction="in"/>
<pin name="CINV+" direction="in"/>
<pin name="VIN_N" direction="in"/>
<pin name="RT"/>
<pin name="EN+" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="BYP+" direction="in"/>
<pin name="ADJ+" direction="in"/>
<pin name="LDO+" direction="in"/>
<pin name="VOUT+" direction="pas"/>
<pin name="GND" direction="in"/>
</symbol>
<symbol name="LTM4622">
<pin name="VOUT2@A1" direction="pas"/>
<pin name="VOUT2@B1" direction="pas"/>
<pin name="GND@C1" direction="in"/>
<pin name="VOUT1@D1" direction="pas"/>
<pin name="VOUT1@E1" direction="pas"/>
<pin name="VIN@A2" direction="in"/>
<pin name="RUN2" direction="in"/>
<pin name="GND@C2" direction="in"/>
<pin name="RUN1" direction="in"/>
<pin name="VIN@E2" direction="in"/>
<pin name="TRACK/SS2" direction="pas"/>
<pin name="VIN@B3" direction="in"/>
<pin name="INTVCC" direction="out"/>
<pin name="VIN@D3" direction="in"/>
<pin name="TRACK/SS1" direction="pas"/>
<pin name="FB2" direction="in"/>
<pin name="PGOOD2" direction="pas"/>
<pin name="FREQ" direction="pas"/>
<pin name="PGOOD1" direction="pas"/>
<pin name="FB1" direction="in"/>
<pin name="COMP2" direction="pas"/>
<pin name="GND@B5" direction="in"/>
<pin name="SYNC/MODE" direction="pas"/>
<pin name="GND@D5" direction="in"/>
<pin name="COMP1" direction="pas"/>
</symbol>
<symbol name="LTC2296">
<pin name="AINA+"/>
<pin name="AINA-"/>
<pin name="REFHA1"/>
<pin name="REFHA2"/>
<pin name="REFLA1"/>
<pin name="REFLA2"/>
<pin name="CLKA" direction="in" function="clk"/>
<pin name="CLKB" direction="in" function="clk"/>
<pin name="REFLB1"/>
<pin name="REFLB2"/>
<pin name="REFHB1"/>
<pin name="REFHB2"/>
<pin name="AINB-"/>
<pin name="AINB+"/>
<pin name="GND1"/>
<pin name="VDD3"/>
<pin name="SENSEB"/>
<pin name="VCMB"/>
<pin name="MUX"/>
<pin name="SHDNB"/>
<pin name="OEB" function="dot"/>
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="OGND1"/>
<pin name="OVDD1"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
<pin name="DB12" direction="out"/>
<pin name="DB13" direction="out"/>
<pin name="OFB" direction="out"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DA12" direction="out"/>
<pin name="DA13" direction="out"/>
<pin name="OFA"/>
<pin name="OEA" function="dot"/>
<pin name="SHDNA"/>
<pin name="MODE"/>
<pin name="VCMA"/>
<pin name="SENSEA"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="OGND2"/>
<pin name="OVDD2"/>
<pin name="VDD4"/>
<pin name="GND2"/>
<pin name="BOTTOM_PAD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LT1129CQ-5" prefix="U" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
</gates>
<devices>
<device name="" package="DDPACK-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CS8" prefix="U" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G$2" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$2" pin="NC" pad="4"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G2" pin="GND" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CT-5" prefix="U" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129"/>
</gates>
<devices>
<device name="" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1129CST5" prefix="U" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt; &lt;p&gt;
with shutdown</description>
<gates>
<gate name="G$1" symbol="LT1129-3"/>
<gate name="GND" symbol="GND"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="GND" pin="GND" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1016" prefix="U" uservalue="yes">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt; Ultra-fast precision</description>
<gates>
<gate name="G$1" symbol="LT1016"/>
</gates>
<devices>
<device name="CS8" package="SO08">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LA_EN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CN" package="DIL08">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LA_EN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1658MS8" prefix="U" uservalue="yes">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LTC1658"/>
</gates>
<devices>
<device name="" package="MSOP08">
<connects>
<connect gate="G$1" pin="!CSLD" pad="3"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1440*" prefix="U">
<description>&lt;b&gt;Comparator&lt;/b&gt; - ultralow power with reference</description>
<gates>
<gate name="G$1" symbol="LTC1440"/>
</gates>
<devices>
<device name="" package="MSOP08">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HYST" pad="5"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1050" prefix="U">
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1764A*" prefix="U">
<description>&lt;b&gt;Regulator&lt;/b&gt; - 3A, LDO, adjustable</description>
<gates>
<gate name="G$1" symbol="LT1764A"/>
</gates>
<devices>
<device name="" package="DDPACK-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="TAB" pad="6"/>
</connects>
<technologies>
<technology name="EQ"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1716" prefix="U">
<description>&lt;b&gt; Comparator, 44V, beyond rail-to-rail, precision, micropower &lt;/b&gt;
&lt;p&gt;
Linear Technology, Digikey part #: LT1716IS5-ND</description>
<gates>
<gate name="G$1" symbol="LT1716"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1512" prefix="U">
<description>&lt;b&gt; Linear Tech-SEPIC CC/CV Battery charger &lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LT1512"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="IFB" pad="3"/>
<connect gate="G$1" pin="S/S" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1370T" prefix="U">
<gates>
<gate name="G$1" symbol="LT1370T"/>
</gates>
<devices>
<device name="" package="DDPACK-7+TAB">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="NFB" pad="6"/>
<connect gate="G$1" pin="S/S" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1370CT7" prefix="U">
<gates>
<gate name="G$1" symbol="LT1370"/>
</gates>
<devices>
<device name="" package="TO220-7">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NFB" pad="6"/>
<connect gate="G$1" pin="S/S" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1025" prefix="U">
<gates>
<gate name="G$1" symbol="LT1025"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="K" pad="7"/>
<connect gate="G$1" pin="R-" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1261L" prefix="U">
<description>&lt;b&gt;VOLTAGE INVERTER&lt;/b&gt; &lt;p&gt;
Switched Capacitor Regulated</description>
<gates>
<gate name="G$1" symbol="LTC1261L"/>
</gates>
<devices>
<device name="CMS8" package="MSOP08">
<connects>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REG" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CS8" package="SO08">
<connects>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REG" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1637" prefix="U">
<description>&lt;b&gt;OP-AMP&lt;/b&gt;&lt;p&gt; Precision 1.1 Mhz, rail-to-rail op-amp</description>
<gates>
<gate name="G$1" symbol="LT1637"/>
</gates>
<devices>
<device name="CMS8" package="MSOP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CS8" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1269" prefix="U">
<description>&lt;b&gt;Switching Regulator&lt;/b&gt; - 4A high efficiency</description>
<gates>
<gate name="G$1" symbol="LT1269"/>
</gates>
<devices>
<device name="CQ" package="DDPACK-5">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT" package="TO220-5">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1910" prefix="U">
<description>&lt;b&gt;High Side MOSFET Driver&lt;/b&gt; - protected</description>
<gates>
<gate name="G$1" symbol="LT1910"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!FAULT!" pad="3"/>
<connect gate="G$1" pin="GATE" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="6"/>
<connect gate="G$1" pin="TIMER" pad="2"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT117XCQ" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT107X"/>
</gates>
<devices>
<device name="" package="TO263-5">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT137P" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="ITC137P"/>
</gates>
<devices>
<device name="" package="SO16W">
<connects>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="BRG" pad="11"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="E" pad="13"/>
<connect gate="G$1" pin="OH+" pad="2"/>
<connect gate="G$1" pin="OH-" pad="3"/>
<connect gate="G$1" pin="RDET" pad="9"/>
<connect gate="G$1" pin="RI+" pad="7"/>
<connect gate="G$1" pin="RI-" pad="8"/>
<connect gate="G$1" pin="RING" pad="10"/>
<connect gate="G$1" pin="T" pad="15"/>
<connect gate="G$1" pin="TIP" pad="16"/>
<connect gate="G$1" pin="Z1" pad="4"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1172" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT117X"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1370CR" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT1370CR"/>
</gates>
<devices>
<device name="" package="TO263-7">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NFB" pad="6"/>
<connect gate="G$1" pin="S/S" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1374CR-5" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT1374"/>
</gates>
<devices>
<device name="" package="TO263-7">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="2"/>
<connect gate="G$1" pin="BOOST" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1513" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT1513"/>
</gates>
<devices>
<device name="" package="TO263-7">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IFB" pad="3"/>
<connect gate="G$1" pin="S/S" pad="6"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VFB" pad="2"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1615" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT1615"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1761-BYP" prefix="U">
<description>&lt;b&gt;Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
adjustable output</description>
<gates>
<gate name="G$1" symbol="LT1761-BYP"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1964" prefix="U">
<description>&lt;b&gt;Negative Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
fixed output with shutdown control</description>
<gates>
<gate name="G$1" symbol="LT1964"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="4"/>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1155" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LTC1155"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="8"/>
<connect gate="G$1" pin="G1" pad="2"/>
<connect gate="G$1" pin="G2" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1732" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LTC1732"/>
</gates>
<devices>
<device name="" package="MS10">
<connects>
<connect gate="G$1" pin="!ACPR!" pad="10"/>
<connect gate="G$1" pin="!CHRG!" pad="3"/>
<connect gate="G$1" pin="BAT" pad="1"/>
<connect gate="G$1" pin="DRV" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="SEL" pad="2"/>
<connect gate="G$1" pin="SENSE" pad="9"/>
<connect gate="G$1" pin="TIMER" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1735" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LT1735"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="BG" pad="11"/>
<connect gate="G$1" pin="BOOST" pad="15"/>
<connect gate="G$1" pin="COSC" pad="1"/>
<connect gate="G$1" pin="EXTVCC" pad="9"/>
<connect gate="G$1" pin="FCB" pad="4"/>
<connect gate="G$1" pin="INTVCC" pad="12"/>
<connect gate="G$1" pin="ITH" pad="3"/>
<connect gate="G$1" pin="PGND" pad="10"/>
<connect gate="G$1" pin="RUN/SS" pad="2"/>
<connect gate="G$1" pin="SENSE+" pad="8"/>
<connect gate="G$1" pin="SENSE-" pad="7"/>
<connect gate="G$1" pin="SGND" pad="5"/>
<connect gate="G$1" pin="SW" pad="14"/>
<connect gate="G$1" pin="TG" pad="16"/>
<connect gate="G$1" pin="VIN" pad="13"/>
<connect gate="G$1" pin="VOSENSE" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1877" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LTC1877"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="ITH" pad="2"/>
<connect gate="G$1" pin="PLL" pad="8"/>
<connect gate="G$1" pin="RUN" pad="1"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="SYNC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="3"/>
<connect gate="G$1" pin="VIN" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3407" prefix="U">
<gates>
<gate name="G$1" symbol="LTC3407"/>
</gates>
<devices>
<device name="" package="MS10-THERM">
<connects>
<connect gate="G$1" pin="!POR!" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="HS" pad="T"/>
<connect gate="G$1" pin="MODE/SYNC" pad="6"/>
<connect gate="G$1" pin="RUN1" pad="2"/>
<connect gate="G$1" pin="RUN2" pad="9"/>
<connect gate="G$1" pin="SW1" pad="4"/>
<connect gate="G$1" pin="SW2" pad="7"/>
<connect gate="G$1" pin="VFB1" pad="1"/>
<connect gate="G$1" pin="VFB2" pad="10"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1620IS8" prefix="U">
<description>&lt;b&gt;CURRENT SENSE AMP&lt;/b&gt;&lt;p&gt; rail-to-rail current sense amp</description>
<gates>
<gate name="G$1" symbol="LT1620IS8"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="AVG" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="IOUT" pad="2"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3800" prefix="U">
<description>&lt;b&gt;Step Down Switcher&lt;/b&gt;&lt;p&gt;
High-Voltage Synchronous Current Mode</description>
<gates>
<gate name="G$1" symbol="LT3800"/>
</gates>
<devices>
<device name="" package="TSSOP16-BC">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="BG" pad="11"/>
<connect gate="G$1" pin="BOOST" pad="16"/>
<connect gate="G$1" pin="BURST_EN" pad="5"/>
<connect gate="G$1" pin="CSS" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC2" pad="13"/>
<connect gate="G$1" pin="PGND" pad="10"/>
<connect gate="G$1" pin="SENSE+" pad="9"/>
<connect gate="G$1" pin="SENSE-" pad="8"/>
<connect gate="G$1" pin="SGND" pad="17"/>
<connect gate="G$1" pin="SW" pad="14"/>
<connect gate="G$1" pin="TG" pad="15"/>
<connect gate="G$1" pin="VC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="6"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT2606" prefix="U">
<description>&lt;b&gt;DAC&lt;/b&gt;&lt;p&gt;
16-/14-/12-Bit Rail-to-Rail with I2C Interface</description>
<gates>
<gate name="G$1" symbol="LT2606"/>
</gates>
<devices>
<device name="" package="DFN10">
<connects>
<connect gate="G$1" pin="!LDAC!" pad="10"/>
<connect gate="G$1" pin="CA0" pad="4"/>
<connect gate="G$1" pin="CA1" pad="5"/>
<connect gate="G$1" pin="CA2" pad="1"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1676" prefix="U">
<description>Step-Down Switching Regulator</description>
<gates>
<gate name="G$1" symbol="LT1676"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="6"/>
<connect gate="G$1" pin="VC" pad="8"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VSW" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3406" prefix="U">
<description>1.5 and 1.8V Step-Down Regulator&lt;p&gt;1.5MHz, 600mA Synchronous</description>
<gates>
<gate name="G$1" symbol="LTC3406"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RUN" pad="1"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3471" prefix="U">
<description>Boost/Inverter&lt;p&gt;
Dual 1.3A, 1.2MHz</description>
<gates>
<gate name="G$1" symbol="LT3471"/>
</gates>
<devices>
<device name="" package="DFN10">
<connects>
<connect gate="G$1" pin="!SHDN1!" pad="9"/>
<connect gate="G$1" pin="!SHDN2!" pad="7"/>
<connect gate="G$1" pin="FB1N" pad="1"/>
<connect gate="G$1" pin="FB1P" pad="2"/>
<connect gate="G$1" pin="FB2N" pad="5"/>
<connect gate="G$1" pin="FB2P" pad="4"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="SW1" pad="10"/>
<connect gate="G$1" pin="SW2" pad="6"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VREF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1761-SD" prefix="U">
<description>&lt;b&gt;Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
adjustable output with shutdown control</description>
<gates>
<gate name="G$1" symbol="LT1761-SD"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1761" prefix="U">
<description>&lt;b&gt;Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
fixed output with shutdown control</description>
<gates>
<gate name="G$1" symbol="LT1761"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1964-BYP" prefix="U">
<description>&lt;b&gt;Negative Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
adjustable output</description>
<gates>
<gate name="G$1" symbol="LT1964-BYP"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1964-SD" prefix="U">
<description>&lt;b&gt;Negative Regulator&lt;/b&gt;&lt;p&gt;
100mA, Low Noise, LDO Micropower&lt;p&gt;
adjustable output with shutdown control</description>
<gates>
<gate name="G$1" symbol="LT1964-SD"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1791" prefix="U">
<description>RS485/RS422 Transceivers&lt;p&gt;
60V Fault Protected</description>
<gates>
<gate name="G$1" symbol="LT1791"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="G$1" pin="!RE!" pad="3"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO14">
<connects>
<connect gate="G$1" pin="!RE!" pad="3"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6241" prefix="U">
<description>&lt;b&gt;OP AMP&lt;/b&gt; - CMOS&lt;p&gt;
18MHz,  Low Noise, Rail-to-Rail Output,</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="S8" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1564" prefix="U">
<description>Antialiasing Filter&lt;p&gt;
Digitally Controlled, 10kHz to 150kHz and 4-Bit P.G.A.</description>
<gates>
<gate name="G$1" symbol="LTC1564"/>
</gates>
<devices>
<device name="" package="SSOP16-5">
<connects>
<connect gate="G$1" pin="!EN!" pad="3"/>
<connect gate="G$1" pin="!RST!" pad="13"/>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="F0" pad="8"/>
<connect gate="G$1" pin="F1" pad="7"/>
<connect gate="G$1" pin="F2" pad="6"/>
<connect gate="G$1" pin="F3" pad="5"/>
<connect gate="G$1" pin="G0" pad="9"/>
<connect gate="G$1" pin="G1" pad="10"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="12"/>
<connect gate="G$1" pin="HOLD" pad="4"/>
<connect gate="G$1" pin="IN" pad="16"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1821">
<gates>
<gate name="G$1" symbol="LTC1821"/>
</gates>
<devices>
<device name="" package="SSOP-36W">
<connects>
<connect gate="G$1" pin="!CLR!" pad="7"/>
<connect gate="G$1" pin="!LD!" pad="23"/>
<connect gate="G$1" pin="!WR!" pad="24"/>
<connect gate="G$1" pin="AGNDF" pad="17"/>
<connect gate="G$1" pin="AGNDS" pad="16"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D10" pad="30"/>
<connect gate="G$1" pin="D11" pad="29"/>
<connect gate="G$1" pin="D12" pad="28"/>
<connect gate="G$1" pin="D13" pad="27"/>
<connect gate="G$1" pin="D14" pad="26"/>
<connect gate="G$1" pin="D15" pad="25"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="D3" pad="3"/>
<connect gate="G$1" pin="D4" pad="36"/>
<connect gate="G$1" pin="D5" pad="35"/>
<connect gate="G$1" pin="D6" pad="34"/>
<connect gate="G$1" pin="D7" pad="33"/>
<connect gate="G$1" pin="D8" pad="32"/>
<connect gate="G$1" pin="D9" pad="31"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="DNC@1" pad="18"/>
<connect gate="G$1" pin="DNC@2" pad="19"/>
<connect gate="G$1" pin="DNC@3" pad="21"/>
<connect gate="G$1" pin="IOUT" pad="14"/>
<connect gate="G$1" pin="NC" pad="22"/>
<connect gate="G$1" pin="R1" pad="10"/>
<connect gate="G$1" pin="RCOM" pad="9"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RFB" pad="12"/>
<connect gate="G$1" pin="ROFS" pad="11"/>
<connect gate="G$1" pin="V+" pad="15"/>
<connect gate="G$1" pin="V-" pad="20"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1460" prefix="U">
<description>Micropower Precision
Series Reference Family</description>
<gates>
<gate name="G$1" symbol="LT1460"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1966" prefix="U">
<description>RMS-to-DC Converter</description>
<gates>
<gate name="G$1" symbol="LTC1966"/>
</gates>
<devices>
<device name="MS8" package="MSOP08">
<connects>
<connect gate="G$1" pin="!EN!" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="OUT-RTN" pad="6"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6905" prefix="U">
<description>CLOCK OSCILLATOR&lt;p&gt;
17-170 MHZ</description>
<gates>
<gate name="G$1" symbol="LTC6905"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="DIV" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="SET" pad="3"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT6650" prefix="U">
<description>&lt;b&gt;Voltage Reference&lt;/b&gt;&lt;p&gt;
Micropower, 400mV Rail-to-Rail</description>
<gates>
<gate name="G$1" symbol="LT6650"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3430" prefix="U">
<description>&lt;b&gt;Switching Regulator&lt;/b&gt;&lt;p&gt;
High Voltage, 3A, 200kHz/100kHz Step-Down</description>
<gates>
<gate name="G$1" symbol="LT3430"/>
</gates>
<devices>
<device name="" package="TSSOP16-BC">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="15"/>
<connect gate="G$1" pin="BIAS" pad="10"/>
<connect gate="G$1" pin="BOOST" pad="6"/>
<connect gate="G$1" pin="FB" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="SW@2" pad="2"/>
<connect gate="G$1" pin="SW@5" pad="5"/>
<connect gate="G$1" pin="SYNC" pad="14"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VIN@3" pad="3"/>
<connect gate="G$1" pin="VIN@4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963AEQ" prefix="U">
<description>&lt;b&gt;LDO Regulator&lt;/b&gt;&lt;p&gt;
1.5A, Low Noise,
Fast Transient Response</description>
<gates>
<gate name="G$1" symbol="1963AEQ"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="TAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1054" prefix="U">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;&lt;p&gt;
Switched Capacitor Voltage Convertor</description>
<gates>
<gate name="G$1" symbol="LT1054"/>
</gates>
<devices>
<device name="S8" package="SO08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="FB/SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="FB/SHDN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1481" prefix="U">
<description>&lt;b&gt;RS485 Transceiver&lt;/b&gt;&lt;p&gt;
Ultralow Power with Shutdown</description>
<gates>
<gate name="G$1" symbol="LTC1481"/>
</gates>
<devices>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S8" package="SO08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3652" prefix="U">
<description>BATTERY CHARGER&lt;p&gt;
Power Tracking 2A for Solar Power</description>
<gates>
<gate name="G$1" symbol="LT3652"/>
</gates>
<devices>
<device name="-DD" package="DFN12-3X3">
<connects>
<connect gate="G$1" pin="!CHRG!" pad="4"/>
<connect gate="G$1" pin="!FAULT!" pad="5"/>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="BAT" pad="9"/>
<connect gate="G$1" pin="BOOST" pad="11"/>
<connect gate="G$1" pin="NTC" pad="8"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="G$1" pin="SW" pad="12"/>
<connect gate="G$1" pin="TIMER" pad="6"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VIN_REG" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MSE" package="MSOP12-MSE">
<connects>
<connect gate="G$1" pin="!CHRG!" pad="4"/>
<connect gate="G$1" pin="!FAULT!" pad="5"/>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="BAT" pad="9"/>
<connect gate="G$1" pin="BOOST" pad="11"/>
<connect gate="G$1" pin="NTC" pad="8"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="G$1" pin="SW" pad="12"/>
<connect gate="G$1" pin="TIMER" pad="6"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VIN_REG" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4411" prefix="U">
<description>Low Loss Ideal Diode 2.6A</description>
<gates>
<gate name="G$1" symbol="LTC4411"/>
</gates>
<devices>
<device name="S5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CTL" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="STAT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2173/74/75" prefix="U">
<description>&lt;b&gt;QUAD ADC&lt;/b&gt;&lt;p&gt;
14-Bit, 125Msps/105Msps/80Msps Low Power</description>
<gates>
<gate name="G$1" symbol="LTC2173/74/75"/>
</gates>
<devices>
<device name="" package="QFN52-UKG">
<connects>
<connect gate="G$1" pin="!CS!" pad="19"/>
<connect gate="G$1" pin="AIN1+" pad="1"/>
<connect gate="G$1" pin="AIN1-" pad="2"/>
<connect gate="G$1" pin="AIN2+" pad="4"/>
<connect gate="G$1" pin="AIN2-" pad="5"/>
<connect gate="G$1" pin="AIN3+" pad="10"/>
<connect gate="G$1" pin="AIN3-" pad="11"/>
<connect gate="G$1" pin="AIN4+" pad="13"/>
<connect gate="G$1" pin="AIN4-" pad="14"/>
<connect gate="G$1" pin="DCO+" pad="36"/>
<connect gate="G$1" pin="DCO-" pad="35"/>
<connect gate="G$1" pin="ENC+" pad="17"/>
<connect gate="G$1" pin="ENC-" pad="18"/>
<connect gate="G$1" pin="FR+" pad="32"/>
<connect gate="G$1" pin="FR-" pad="31"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@45" pad="45"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="OGND" pad="33"/>
<connect gate="G$1" pin="OUT1A+" pad="44"/>
<connect gate="G$1" pin="OUT1A-" pad="43"/>
<connect gate="G$1" pin="OUT1B+" pad="42"/>
<connect gate="G$1" pin="OUT1B-" pad="41"/>
<connect gate="G$1" pin="OUT2A+" pad="40"/>
<connect gate="G$1" pin="OUT2A-" pad="39"/>
<connect gate="G$1" pin="OUT2B+" pad="38"/>
<connect gate="G$1" pin="OUT2B-" pad="37"/>
<connect gate="G$1" pin="OUT3A+" pad="30"/>
<connect gate="G$1" pin="OUT3A-" pad="29"/>
<connect gate="G$1" pin="OUT3B+" pad="28"/>
<connect gate="G$1" pin="OUT3B-" pad="27"/>
<connect gate="G$1" pin="OUT4A+" pad="26"/>
<connect gate="G$1" pin="OUT4A-" pad="25"/>
<connect gate="G$1" pin="OUT4B+" pad="24"/>
<connect gate="G$1" pin="OUT4B-" pad="23"/>
<connect gate="G$1" pin="OVDD" pad="34"/>
<connect gate="G$1" pin="PAR/!SER!" pad="47"/>
<connect gate="G$1" pin="REFH@6" pad="6"/>
<connect gate="G$1" pin="REFH@7" pad="7"/>
<connect gate="G$1" pin="REFL@8" pad="8"/>
<connect gate="G$1" pin="REFL@9" pad="9"/>
<connect gate="G$1" pin="SCK" pad="20"/>
<connect gate="G$1" pin="SDI" pad="21"/>
<connect gate="G$1" pin="SDO" pad="46"/>
<connect gate="G$1" pin="SENSE" pad="50"/>
<connect gate="G$1" pin="VCM12" pad="3"/>
<connect gate="G$1" pin="VCM34" pad="12"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@16" pad="16"/>
<connect gate="G$1" pin="VDD@51" pad="51"/>
<connect gate="G$1" pin="VDD@52" pad="52"/>
<connect gate="G$1" pin="VREF" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4412" prefix="U">
<description>Low Loss PowerPath Controller</description>
<gates>
<gate name="G$1" symbol="LTC4412"/>
</gates>
<devices>
<device name="" package="TSOT23-6">
<connects>
<connect gate="G$1" pin="CTL" pad="3"/>
<connect gate="G$1" pin="GATE" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SENSE" pad="6"/>
<connect gate="G$1" pin="STAT" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1763" prefix="U">
<description>&lt;b&gt;LDO REGULATOR&lt;/b&gt;&lt;p&gt;
500mA, Low Noise, Micropower</description>
<gates>
<gate name="G$1" symbol="LT1763"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="5"/>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SEN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4357" prefix="U">
<description>&lt;b&gt;IDEAL DIODE CONTROLLER&lt;/b&gt;&lt;p&gt;
Positive High Voltage Ideal Diode Controller</description>
<gates>
<gate name="G$1" symbol="LTC4357"/>
</gates>
<devices>
<device name="MS8" package="MSOP08">
<connects>
<connect gate="G$1" pin="GATE" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCB" package="DFN6-2X3">
<connects>
<connect gate="G$1" pin="GATE" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC485" prefix="U">
<description>RS485 TRANSCIEVER</description>
<gates>
<gate name="G$1" symbol="LTC485"/>
</gates>
<devices>
<device name="S8" package="SO08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="!RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTM8022" prefix="U">
<description>DC/DC CONVERTOR&lt;p&gt;
step-down, 1A, 36V DC/DC uModule</description>
<gates>
<gate name="G$1" symbol="LTM8022"/>
</gates>
<devices>
<device name="" package="LGA50-SMD">
<connects>
<connect gate="G$1" pin="ADJ" pad="H7"/>
<connect gate="G$1" pin="AUX" pad="F5"/>
<connect gate="G$1" pin="BIAS" pad="G5"/>
<connect gate="G$1" pin="GND@A5" pad="A5"/>
<connect gate="G$1" pin="GND@A6" pad="A6"/>
<connect gate="G$1" pin="GND@A7" pad="A7"/>
<connect gate="G$1" pin="GND@B5" pad="B5"/>
<connect gate="G$1" pin="GND@B6" pad="B6"/>
<connect gate="G$1" pin="GND@B7" pad="B7"/>
<connect gate="G$1" pin="GND@C5" pad="C5"/>
<connect gate="G$1" pin="GND@C6" pad="C6"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@D1" pad="D1"/>
<connect gate="G$1" pin="GND@D2" pad="D2"/>
<connect gate="G$1" pin="GND@D3" pad="D3"/>
<connect gate="G$1" pin="GND@D4" pad="D4"/>
<connect gate="G$1" pin="GND@D5" pad="D5"/>
<connect gate="G$1" pin="GND@D6" pad="D6"/>
<connect gate="G$1" pin="GND@D7" pad="D7"/>
<connect gate="G$1" pin="GND@E1" pad="E1"/>
<connect gate="G$1" pin="GND@E2" pad="E2"/>
<connect gate="G$1" pin="GND@E3" pad="E3"/>
<connect gate="G$1" pin="GND@E4" pad="E4"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E6" pad="E6"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@F6" pad="F6"/>
<connect gate="G$1" pin="IN@G1" pad="G1"/>
<connect gate="G$1" pin="IN@G2" pad="G2"/>
<connect gate="G$1" pin="IN@G3" pad="G3"/>
<connect gate="G$1" pin="IN@H1" pad="H1"/>
<connect gate="G$1" pin="IN@H2" pad="H2"/>
<connect gate="G$1" pin="IN@H3" pad="H3"/>
<connect gate="G$1" pin="OUT@A1" pad="A1"/>
<connect gate="G$1" pin="OUT@A2" pad="A2"/>
<connect gate="G$1" pin="OUT@A3" pad="A3"/>
<connect gate="G$1" pin="OUT@A4" pad="A4"/>
<connect gate="G$1" pin="OUT@B1" pad="B1"/>
<connect gate="G$1" pin="OUT@B2" pad="B2"/>
<connect gate="G$1" pin="OUT@B3" pad="B3"/>
<connect gate="G$1" pin="OUT@B4" pad="B4"/>
<connect gate="G$1" pin="OUT@C1" pad="C1"/>
<connect gate="G$1" pin="OUT@C2" pad="C2"/>
<connect gate="G$1" pin="OUT@C3" pad="C3"/>
<connect gate="G$1" pin="OUT@C4" pad="C4"/>
<connect gate="G$1" pin="PG" pad="H6"/>
<connect gate="G$1" pin="RT" pad="G7"/>
<connect gate="G$1" pin="RUN/SS" pad="H5"/>
<connect gate="G$1" pin="SHARE" pad="F7"/>
<connect gate="G$1" pin="SYNC" pad="G6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6102" prefix="U">
<description>&lt;b&gt;Current Sense Amplifier&lt;/b&gt;&lt;p&gt;
Precision Zero Drift</description>
<gates>
<gate name="G$1" symbol="LTC6102"/>
</gates>
<devices>
<device name="MS8" package="MSOP08">
<connects>
<connect gate="G$1" pin="+IN" pad="8"/>
<connect gate="G$1" pin="-INF" pad="2"/>
<connect gate="G$1" pin="-INS" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="5"/>
<connect gate="G$1" pin="V-/EN" pad="3"/>
<connect gate="G$1" pin="VREG" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DD" package="DFN8-3X3">
<connects>
<connect gate="G$1" pin="+IN" pad="8"/>
<connect gate="G$1" pin="-INF" pad="2"/>
<connect gate="G$1" pin="-INS" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="5"/>
<connect gate="G$1" pin="V-/EN" pad="3"/>
<connect gate="G$1" pin="VREG" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4413-2" prefix="U">
<description>2-Channel Ideal OR'ing Diode&lt;p&gt;
Dual 2.6A, 2.5V to 5.5V</description>
<gates>
<gate name="G$1" symbol="LTC4413-2"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="ENBA" pad="2"/>
<connect gate="G$1" pin="ENBB" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="INA" pad="1"/>
<connect gate="G$1" pin="INB" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="10"/>
<connect gate="G$1" pin="OUTB" pad="6"/>
<connect gate="G$1" pin="OVI" pad="8"/>
<connect gate="G$1" pin="OVP" pad="7"/>
<connect gate="G$1" pin="STAT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4413-1" prefix="U">
<description>2-Channel Ideal OR'ing Diode&lt;p&gt;
Dual 2.6A, 2.5V to 5.5V</description>
<gates>
<gate name="G$1" symbol="LTC4413-1"/>
</gates>
<devices>
<device name="" package="DFN10-3X3">
<connects>
<connect gate="G$1" pin="ENBA" pad="2"/>
<connect gate="G$1" pin="ENBB" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="INA" pad="1"/>
<connect gate="G$1" pin="INB" pad="5"/>
<connect gate="G$1" pin="NC@7" pad="7"/>
<connect gate="G$1" pin="NC@8" pad="8"/>
<connect gate="G$1" pin="OUTA" pad="10"/>
<connect gate="G$1" pin="OUTB" pad="6"/>
<connect gate="G$1" pin="STAT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2266/67/68-14" prefix="U">
<description>&lt;b&gt;DUAL ADC&lt;/b&gt;&lt;p&gt;
14-Bit, 125Msps/105Msps/80Msps Low Power</description>
<gates>
<gate name="G$1" symbol="LTC2266/67/68-14"/>
</gates>
<devices>
<device name="" package="QFN40-UJ">
<connects>
<connect gate="G$1" pin="!CS!" pad="15"/>
<connect gate="G$1" pin="AIN1+" pad="1"/>
<connect gate="G$1" pin="AIN1-" pad="2"/>
<connect gate="G$1" pin="AIN2+" pad="9"/>
<connect gate="G$1" pin="AIN2-" pad="10"/>
<connect gate="G$1" pin="DCO+" pad="28"/>
<connect gate="G$1" pin="DCO-" pad="27"/>
<connect gate="G$1" pin="ENC+" pad="13"/>
<connect gate="G$1" pin="ENC-" pad="14"/>
<connect gate="G$1" pin="FR+" pad="24"/>
<connect gate="G$1" pin="FR-" pad="23"/>
<connect gate="G$1" pin="GND@$33" pad="33"/>
<connect gate="G$1" pin="GND@13" pad="18"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="OGND" pad="25"/>
<connect gate="G$1" pin="OUT1A+" pad="32"/>
<connect gate="G$1" pin="OUT1A-" pad="31"/>
<connect gate="G$1" pin="OUT1B+" pad="30"/>
<connect gate="G$1" pin="OUT1B-" pad="29"/>
<connect gate="G$1" pin="OUT2A+" pad="22"/>
<connect gate="G$1" pin="OUT2A-" pad="21"/>
<connect gate="G$1" pin="OUT2B+" pad="20"/>
<connect gate="G$1" pin="OUT2B-" pad="19"/>
<connect gate="G$1" pin="OVDD" pad="26"/>
<connect gate="G$1" pin="PAR/!SER!" pad="35"/>
<connect gate="G$1" pin="REFH@4" pad="4"/>
<connect gate="G$1" pin="REFH@5" pad="5"/>
<connect gate="G$1" pin="REFL@6" pad="6"/>
<connect gate="G$1" pin="REFL@7" pad="7"/>
<connect gate="G$1" pin="SCK" pad="16"/>
<connect gate="G$1" pin="SDI" pad="17"/>
<connect gate="G$1" pin="SDO" pad="34"/>
<connect gate="G$1" pin="SENSE" pad="38"/>
<connect gate="G$1" pin="VCM1" pad="3"/>
<connect gate="G$1" pin="VCM2" pad="8"/>
<connect gate="G$1" pin="VDD@11" pad="11"/>
<connect gate="G$1" pin="VDD@12" pad="12"/>
<connect gate="G$1" pin="VDD@39" pad="39"/>
<connect gate="G$1" pin="VDD@40" pad="40"/>
<connect gate="G$1" pin="VREF" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3601UD" prefix="U">
<description>Synchronous Step-Down Regulator&lt;p&gt;
1.5A, 15V Monolithic</description>
<gates>
<gate name="G$1" symbol="LTC3601UD"/>
</gates>
<devices>
<device name="" package="QFN16-UD">
<connects>
<connect gate="G$1" pin="BOOST" pad="6"/>
<connect gate="G$1" pin="FB" pad="11"/>
<connect gate="G$1" pin="INTVCC" pad="7"/>
<connect gate="G$1" pin="ITH" pad="12"/>
<connect gate="G$1" pin="MODE/SYNC" pad="1"/>
<connect gate="G$1" pin="NC@5" pad="5"/>
<connect gate="G$1" pin="PGOOD" pad="2"/>
<connect gate="G$1" pin="RT" pad="10"/>
<connect gate="G$1" pin="RUN" pad="14"/>
<connect gate="G$1" pin="SGND" pad="9"/>
<connect gate="G$1" pin="SW@3" pad="3"/>
<connect gate="G$1" pin="SW@4" pad="4"/>
<connect gate="G$1" pin="TRACK" pad="13"/>
<connect gate="G$1" pin="VIN@15" pad="15"/>
<connect gate="G$1" pin="VIN@16" pad="16"/>
<connect gate="G$1" pin="VON" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3601MSE" prefix="U">
<description>Synchronous Step-Down Regulator&lt;p&gt;
1.5A, 15V Monolithic</description>
<gates>
<gate name="G$1" symbol="LTC3601MSE"/>
</gates>
<devices>
<device name="" package="MSOP16-MSE">
<connects>
<connect gate="G$1" pin="BOOST" pad="5"/>
<connect gate="G$1" pin="FB" pad="9"/>
<connect gate="G$1" pin="INTVCC" pad="6"/>
<connect gate="G$1" pin="ITH" pad="10"/>
<connect gate="G$1" pin="MODE/SYNC" pad="15"/>
<connect gate="G$1" pin="PGND@3" pad="3"/>
<connect gate="G$1" pin="PGND@4" pad="4"/>
<connect gate="G$1" pin="PGOOD" pad="16"/>
<connect gate="G$1" pin="RT" pad="8"/>
<connect gate="G$1" pin="RUN" pad="12"/>
<connect gate="G$1" pin="SW@1" pad="1"/>
<connect gate="G$1" pin="SW@2" pad="2"/>
<connect gate="G$1" pin="TRACK" pad="11"/>
<connect gate="G$1" pin="VIN@13" pad="13"/>
<connect gate="G$1" pin="VIN@14" pad="14"/>
<connect gate="G$1" pin="VON" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT5534" prefix="U">
<description>RF Power Detector&lt;p&gt;
50MHz to 3GHz, 60dB Dynamic Range</description>
<gates>
<gate name="G$1" symbol="LT5534"/>
</gates>
<devices>
<device name="" package="SC70-6W">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="RF" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6409" prefix="U">
<description>Differential Amplifier/ADC Driver</description>
<gates>
<gate name="G$1" symbol="LTC6409"/>
</gates>
<devices>
<device name="" package="QFN10-UDB">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="3"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+OUT" pad="7"/>
<connect gate="G$1" pin="-IN" pad="6"/>
<connect gate="G$1" pin="-OUT" pad="1"/>
<connect gate="G$1" pin="V+@4" pad="4"/>
<connect gate="G$1" pin="V+@9" pad="9"/>
<connect gate="G$1" pin="V-@10" pad="10"/>
<connect gate="G$1" pin="V-@11" pad="11"/>
<connect gate="G$1" pin="V-@8" pad="8"/>
<connect gate="G$1" pin="VOCM" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3092" prefix="U">
<description>Very Low Dropout
Linear Regulator</description>
<gates>
<gate name="G$1" symbol="LT3092"/>
</gates>
<devices>
<device name="" package="DFN8-3X3">
<connects>
<connect gate="G$1" pin="IN@7" pad="7"/>
<connect gate="G$1" pin="IN@8" pad="8"/>
<connect gate="G$1" pin="OUT@1" pad="1"/>
<connect gate="G$1" pin="OUT@2" pad="2"/>
<connect gate="G$1" pin="OUT@9" pad="9"/>
<connect gate="G$1" pin="SET" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1799" prefix="U">
<description>PRECISION OSCILLATOR</description>
<gates>
<gate name="G$1" symbol="LTC1799"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="DIV" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="SET" pad="3"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2954" prefix="U">
<description>PUSHBUTTON ON/OFF CONTROLLER</description>
<gates>
<gate name="G$1" symbol="LTC2954"/>
</gates>
<devices>
<device name="DDB" package="DFN8-DDB">
<connects>
<connect gate="G$1" pin="!EN!" pad="7"/>
<connect gate="G$1" pin="!INT!" pad="8"/>
<connect gate="G$1" pin="!KILL!" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="ONT" pad="2"/>
<connect gate="G$1" pin="PB" pad="3"/>
<connect gate="G$1" pin="PDT" pad="6"/>
<connect gate="G$1" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4099" prefix="U">
<description>USB Power Manager/Charger</description>
<gates>
<gate name="G$1" symbol="LTC4099"/>
</gates>
<devices>
<device name="" package="QFN20-UDC">
<connects>
<connect gate="G$1" pin="!ACPR!" pad="18"/>
<connect gate="G$1" pin="!IRQ!" pad="8"/>
<connect gate="G$1" pin="BAT" pad="11"/>
<connect gate="G$1" pin="BATSENS" pad="6"/>
<connect gate="G$1" pin="CLPROG" pad="19"/>
<connect gate="G$1" pin="DVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="IDGATE" pad="10"/>
<connect gate="G$1" pin="NTC" pad="2"/>
<connect gate="G$1" pin="NTCBIAS" pad="3"/>
<connect gate="G$1" pin="OVGATE" pad="1"/>
<connect gate="G$1" pin="OVSENS" pad="20"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="17"/>
<connect gate="G$1" pin="SW" pad="14"/>
<connect gate="G$1" pin="VBUS" pad="13"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="12"/>
<connect gate="G$1" pin="WALL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2953" prefix="U">
<description>Push Button On/Off Controller</description>
<gates>
<gate name="G$1" symbol="LTC2953"/>
</gates>
<devices>
<device name="" package="DFN12-3X3">
<connects>
<connect gate="G$1" pin="!INT!" pad="12"/>
<connect gate="G$1" pin="!KILL!" pad="3"/>
<connect gate="G$1" pin="!PB!" pad="5"/>
<connect gate="G$1" pin="!PFI!" pad="8"/>
<connect gate="G$1" pin="!PFO!" pad="9"/>
<connect gate="G$1" pin="!RST!" pad="10"/>
<connect gate="G$1" pin="EN/!EN!" pad="11"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PDT" pad="4"/>
<connect gate="G$1" pin="UVLO" pad="7"/>
<connect gate="G$1" pin="VIN" pad="6"/>
<connect gate="G$1" pin="VM" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2942-1" prefix="U">
<description>1A Battery Gas Gauge&lt;p&gt;
Internal Sense Resistor and Temperature/Voltage Measurement</description>
<gates>
<gate name="G$1" symbol="LTC2942-1"/>
</gates>
<devices>
<device name="" package="DFN6-2X3">
<connects>
<connect gate="G$1" pin="!AL!/CC" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SENSE+" pad="1"/>
<connect gate="G$1" pin="SENSE-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTM2882" prefix="U">
<description>Dual Isolated RS232 Transceiver&lt;p&gt;
uModule + Power</description>
<gates>
<gate name="G$1" symbol="LTM2882"/>
</gates>
<devices>
<device name="" package="BLGA32">
<connects>
<connect gate="G$1" pin="DE" pad="L6"/>
<connect gate="G$1" pin="DIN" pad="A5"/>
<connect gate="G$1" pin="DOUT" pad="L5"/>
<connect gate="G$1" pin="GBD@B2" pad="B2"/>
<connect gate="G$1" pin="GND2@K1" pad="K1"/>
<connect gate="G$1" pin="GND2@K2" pad="K2"/>
<connect gate="G$1" pin="GND2@K3" pad="K3"/>
<connect gate="G$1" pin="GND2@K4" pad="K4"/>
<connect gate="G$1" pin="GND2@K5" pad="K5"/>
<connect gate="G$1" pin="GND2@K6" pad="K6"/>
<connect gate="G$1" pin="GND2@K7" pad="K7"/>
<connect gate="G$1" pin="GND@B1" pad="B1"/>
<connect gate="G$1" pin="GND@B3" pad="B3"/>
<connect gate="G$1" pin="GND@B4" pad="B4"/>
<connect gate="G$1" pin="GND@B5" pad="B5"/>
<connect gate="G$1" pin="GND@B6" pad="B6"/>
<connect gate="G$1" pin="ON" pad="A6"/>
<connect gate="G$1" pin="R1IN" pad="L3"/>
<connect gate="G$1" pin="R1OUT" pad="A3"/>
<connect gate="G$1" pin="R2IN" pad="L1"/>
<connect gate="G$1" pin="R2OUT" pad="A1"/>
<connect gate="G$1" pin="T1IN" pad="A4"/>
<connect gate="G$1" pin="T1OUT" pad="L4"/>
<connect gate="G$1" pin="T2IN" pad="A2"/>
<connect gate="G$1" pin="T2OUT" pad="L2"/>
<connect gate="G$1" pin="VCC2@K8" pad="K8"/>
<connect gate="G$1" pin="VCC2@L7" pad="L7"/>
<connect gate="G$1" pin="VCC2@L8" pad="L8"/>
<connect gate="G$1" pin="VCC@A8" pad="A8"/>
<connect gate="G$1" pin="VCC@B7" pad="B7"/>
<connect gate="G$1" pin="VCC@B8" pad="B8"/>
<connect gate="G$1" pin="VL" pad="A7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2935" prefix="U">
<description>Ultra-Low Power Supervisor&lt;p&gt;
with Power-Fail Output, Selectable Thresholds</description>
<gates>
<gate name="G$1" symbol="LTC2935"/>
</gates>
<devices>
<device name="TS8" package="SOT23-8">
<connects>
<connect gate="G$1" pin="!MR!" pad="7"/>
<connect gate="G$1" pin="!PFO!" pad="5"/>
<connect gate="G$1" pin="!RST!" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="S0" pad="3"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DC" package="DFN8-DC">
<connects>
<connect gate="G$1" pin="!MR!" pad="2"/>
<connect gate="G$1" pin="!PFO!" pad="4"/>
<connect gate="G$1" pin="!RST!" pad="3"/>
<connect gate="G$1" pin="GND" pad="5 9"/>
<connect gate="G$1" pin="S0" pad="6"/>
<connect gate="G$1" pin="S1" pad="7"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1762-ADJ" prefix="U">
<description>&lt;b&gt;LDO REGULATOR&lt;/b&gt;&lt;p&gt;
150mA, Low Noise, Micropower</description>
<gates>
<gate name="G$1" symbol="LT1762-ADJ"/>
</gates>
<devices>
<device name="" package="MSOP08">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="5"/>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC5507" prefix="U">
<description>RF Power Detector</description>
<gates>
<gate name="G$1" symbol="LTC5507"/>
</gates>
<devices>
<device name="" package="TSOT23-6">
<connects>
<connect gate="G$1" pin="!SHDN!" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PCAP" pad="5"/>
<connect gate="G$1" pin="RFIN" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3748" prefix="U">
<description>Isolated Flyback Controller</description>
<gates>
<gate name="G$1" symbol="LT3748"/>
</gates>
<devices>
<device name="" package="MSOP16-MS16(12)">
<connects>
<connect gate="G$1" pin="EN/UVLO" pad="3"/>
<connect gate="G$1" pin="GATE" pad="6"/>
<connect gate="G$1" pin="GND" pad="8 9"/>
<connect gate="G$1" pin="INTVCC" pad="5"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="RREF" pad="14"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="SS" pad="10"/>
<connect gate="G$1" pin="TC" pad="12"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3015" prefix="U">
<description>&lt;b&gt;LDO REGULATOR&lt;/b&gt;&lt;p&gt;
1.5A, Low Noise, Negative Linear Regulator with Precision Current Limit</description>
<gates>
<gate name="G$1" symbol="LT3015-ADJ"/>
</gates>
<devices>
<device name="T" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1963" prefix="U">
<description>&lt;b&gt;LDO Regulator&lt;/b&gt;&lt;p&gt;
1.5A, Low Noise, Fast Transient Response</description>
<gates>
<gate name="G$1" symbol="LT1963A"/>
</gates>
<devices>
<device name="T" package="TO220-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3080" prefix="U">
<description>&lt;b&gt;LDO REGULATOR&lt;/b&gt;&lt;p&gt;
Adjustable1.1A Single Resistor Low Dropout Regulator</description>
<gates>
<gate name="G$1" symbol="LT3080"/>
</gates>
<devices>
<device name="T" package="TO220-5">
<connects>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SET" pad="2"/>
<connect gate="G$1" pin="VCTL" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1962" prefix="U">
<description>LDO REGULATOR</description>
<gates>
<gate name="G$1" symbol="LT1962"/>
</gates>
<devices>
<device name="" package="MSOP08">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="BYP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE/ADJ" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT8471" prefix="U">
<description>&lt;b&gt;DC/DC Converters&lt;/b&gt;&lt;p&gt;
Dual Multitopology with 2A Switches and Synchronization</description>
<gates>
<gate name="G$1" symbol="LT8471"/>
</gates>
<devices>
<device name="" package="TSSOP20-CB">
<connects>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="20"/>
<connect gate="G$1" pin="C3" pad="13"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="19"/>
<connect gate="G$1" pin="FB1" pad="5"/>
<connect gate="G$1" pin="FB2" pad="16"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="OV/UV" pad="6"/>
<connect gate="G$1" pin="PG1" pad="4"/>
<connect gate="G$1" pin="PG2" pad="17"/>
<connect gate="G$1" pin="RT" pad="7"/>
<connect gate="G$1" pin="SHOUT" pad="14"/>
<connect gate="G$1" pin="SS1" pad="8"/>
<connect gate="G$1" pin="SS2" pad="15"/>
<connect gate="G$1" pin="SYNC" pad="9"/>
<connect gate="G$1" pin="VIN1" pad="3"/>
<connect gate="G$1" pin="VIN2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4011" prefix="U">
<description>Nickel Battery Charger</description>
<gates>
<gate name="G$1" symbol="LTC4011"/>
</gates>
<devices>
<device name="" package="TSSOP20-CB">
<connects>
<connect gate="G$1" pin="!CHRG!" pad="3"/>
<connect gate="G$1" pin="!FAULT!" pad="2"/>
<connect gate="G$1" pin="!READY!" pad="19"/>
<connect gate="G$1" pin="!TOC!" pad="13"/>
<connect gate="G$1" pin="BAT" pad="12"/>
<connect gate="G$1" pin="BGATE" pad="15"/>
<connect gate="G$1" pin="CHEM" pad="4"/>
<connect gate="G$1" pin="DCIN" pad="1"/>
<connect gate="G$1" pin="EXPAD" pad="21"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="INFET" pad="20"/>
<connect gate="G$1" pin="INTVDD" pad="14"/>
<connect gate="G$1" pin="PGND" pad="16"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="TGATE" pad="17"/>
<connect gate="G$1" pin="TIMER" pad="10"/>
<connect gate="G$1" pin="VCC" pad="18"/>
<connect gate="G$1" pin="VCDIV" pad="9"/>
<connect gate="G$1" pin="VCELL" pad="8"/>
<connect gate="G$1" pin="VRT" pad="6"/>
<connect gate="G$1" pin="VTEMP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4365" prefix="U">
<description>&lt;b&gt;Supply Protection Controller&lt;/b&gt;&lt;p&gt;
Overvoltage, Undervoltage and Reverse</description>
<gates>
<gate name="G$1" symbol="LTC4365"/>
</gates>
<devices>
<device name="TS8" package="TSOT23-8">
<connects>
<connect gate="G$1" pin="!FAULT!" pad="6"/>
<connect gate="G$1" pin="!SHDN!" pad="5"/>
<connect gate="G$1" pin="0V" pad="3"/>
<connect gate="G$1" pin="GATE" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="UV" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3265" prefix="U">
<description>Low Noise Dual Supply&lt;p&gt;
with Boost and Inverting Charge Pumps</description>
<gates>
<gate name="G$1" symbol="LTC3265"/>
</gates>
<devices>
<device name="DHC" package="DFN18">
<connects>
<connect gate="G$1" pin="ADJ+" pad="16"/>
<connect gate="G$1" pin="ADJ-" pad="6"/>
<connect gate="G$1" pin="BYP+" pad="15"/>
<connect gate="G$1" pin="BYP-" pad="5"/>
<connect gate="G$1" pin="CBST+" pad="2"/>
<connect gate="G$1" pin="CBST-" pad="1"/>
<connect gate="G$1" pin="CINV+" pad="10"/>
<connect gate="G$1" pin="CINV-" pad="9"/>
<connect gate="G$1" pin="EN+" pad="13"/>
<connect gate="G$1" pin="EN-" pad="4"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="LDO+" pad="17"/>
<connect gate="G$1" pin="LDO-" pad="7"/>
<connect gate="G$1" pin="MODE" pad="14"/>
<connect gate="G$1" pin="RT" pad="12"/>
<connect gate="G$1" pin="VIN_N" pad="11"/>
<connect gate="G$1" pin="VIN_P" pad="3"/>
<connect gate="G$1" pin="VOUT+" pad="18"/>
<connect gate="G$1" pin="VOUT-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FE" package="TSSOP20-CB">
<connects>
<connect gate="G$1" pin="ADJ+" pad="18"/>
<connect gate="G$1" pin="ADJ-" pad="7"/>
<connect gate="G$1" pin="BYP+" pad="17"/>
<connect gate="G$1" pin="BYP-" pad="6"/>
<connect gate="G$1" pin="CBST+" pad="3"/>
<connect gate="G$1" pin="CBST-" pad="2"/>
<connect gate="G$1" pin="CINV+" pad="12"/>
<connect gate="G$1" pin="CINV-" pad="10"/>
<connect gate="G$1" pin="EN+" pad="15"/>
<connect gate="G$1" pin="EN-" pad="5"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="LDO+" pad="19"/>
<connect gate="G$1" pin="LDO-" pad="8"/>
<connect gate="G$1" pin="MODE" pad="16"/>
<connect gate="G$1" pin="RT" pad="14"/>
<connect gate="G$1" pin="VIN_N" pad="13"/>
<connect gate="G$1" pin="VIN_P" pad="4"/>
<connect gate="G$1" pin="VOUT+" pad="20"/>
<connect gate="G$1" pin="VOUT-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTM4622" prefix="U">
<description>&lt;b&gt;DC DC CONVERTER&lt;/b&gt;&lt;p&gt;
0.6-5.5V 2.5A</description>
<gates>
<gate name="G$1" symbol="LTM4622"/>
</gates>
<devices>
<device name="Y" package="BGA25">
<connects>
<connect gate="G$1" pin="COMP1" pad="E5"/>
<connect gate="G$1" pin="COMP2" pad="A5"/>
<connect gate="G$1" pin="FB1" pad="E4"/>
<connect gate="G$1" pin="FB2" pad="A4"/>
<connect gate="G$1" pin="FREQ" pad="C4"/>
<connect gate="G$1" pin="GND@B5" pad="B5"/>
<connect gate="G$1" pin="GND@C1" pad="C1"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@D5" pad="D5"/>
<connect gate="G$1" pin="INTVCC" pad="C3"/>
<connect gate="G$1" pin="PGOOD1" pad="D4"/>
<connect gate="G$1" pin="PGOOD2" pad="B4"/>
<connect gate="G$1" pin="RUN1" pad="D2"/>
<connect gate="G$1" pin="RUN2" pad="B2"/>
<connect gate="G$1" pin="SYNC/MODE" pad="C5"/>
<connect gate="G$1" pin="TRACK/SS1" pad="E3"/>
<connect gate="G$1" pin="TRACK/SS2" pad="A3"/>
<connect gate="G$1" pin="VIN@A2" pad="A2"/>
<connect gate="G$1" pin="VIN@B3" pad="B3"/>
<connect gate="G$1" pin="VIN@D3" pad="D3"/>
<connect gate="G$1" pin="VIN@E2" pad="E2"/>
<connect gate="G$1" pin="VOUT1@D1" pad="D1"/>
<connect gate="G$1" pin="VOUT1@E1" pad="E1"/>
<connect gate="G$1" pin="VOUT2@A1" pad="A1"/>
<connect gate="G$1" pin="VOUT2@B1" pad="B1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2296">
<gates>
<gate name="G$1" symbol="LTC2296"/>
</gates>
<devices>
<device name="" package="QFN-64">
<connects>
<connect gate="G$1" pin="AINA+" pad="1"/>
<connect gate="G$1" pin="AINA-" pad="2"/>
<connect gate="G$1" pin="AINB+" pad="16"/>
<connect gate="G$1" pin="AINB-" pad="15"/>
<connect gate="G$1" pin="BOTTOM_PAD" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25"/>
<connect gate="G$1" pin="CLKA" pad="8"/>
<connect gate="G$1" pin="CLKB" pad="9"/>
<connect gate="G$1" pin="DA0" pad="41"/>
<connect gate="G$1" pin="DA1" pad="42"/>
<connect gate="G$1" pin="DA10" pad="53"/>
<connect gate="G$1" pin="DA11" pad="54"/>
<connect gate="G$1" pin="DA12" pad="55"/>
<connect gate="G$1" pin="DA13" pad="56"/>
<connect gate="G$1" pin="DA2" pad="43"/>
<connect gate="G$1" pin="DA3" pad="44"/>
<connect gate="G$1" pin="DA4" pad="45"/>
<connect gate="G$1" pin="DA5" pad="46"/>
<connect gate="G$1" pin="DA6" pad="47"/>
<connect gate="G$1" pin="DA7" pad="48"/>
<connect gate="G$1" pin="DA8" pad="51"/>
<connect gate="G$1" pin="DA9" pad="52"/>
<connect gate="G$1" pin="DB0" pad="24"/>
<connect gate="G$1" pin="DB1" pad="25"/>
<connect gate="G$1" pin="DB10" pad="36"/>
<connect gate="G$1" pin="DB11" pad="37"/>
<connect gate="G$1" pin="DB12" pad="38"/>
<connect gate="G$1" pin="DB13" pad="39"/>
<connect gate="G$1" pin="DB2" pad="26"/>
<connect gate="G$1" pin="DB3" pad="27"/>
<connect gate="G$1" pin="DB4" pad="28"/>
<connect gate="G$1" pin="DB5" pad="29"/>
<connect gate="G$1" pin="DB6" pad="30"/>
<connect gate="G$1" pin="DB7" pad="33"/>
<connect gate="G$1" pin="DB8" pad="34"/>
<connect gate="G$1" pin="DB9" pad="35"/>
<connect gate="G$1" pin="GND1" pad="17"/>
<connect gate="G$1" pin="GND2" pad="64"/>
<connect gate="G$1" pin="MODE" pad="60"/>
<connect gate="G$1" pin="MUX" pad="21"/>
<connect gate="G$1" pin="OEA" pad="58"/>
<connect gate="G$1" pin="OEB" pad="23"/>
<connect gate="G$1" pin="OFA" pad="57"/>
<connect gate="G$1" pin="OFB" pad="40"/>
<connect gate="G$1" pin="OGND1" pad="31"/>
<connect gate="G$1" pin="OGND2" pad="50"/>
<connect gate="G$1" pin="OVDD1" pad="32"/>
<connect gate="G$1" pin="OVDD2" pad="49"/>
<connect gate="G$1" pin="REFHA1" pad="3"/>
<connect gate="G$1" pin="REFHA2" pad="4"/>
<connect gate="G$1" pin="REFHB1" pad="13"/>
<connect gate="G$1" pin="REFHB2" pad="14"/>
<connect gate="G$1" pin="REFLA1" pad="5"/>
<connect gate="G$1" pin="REFLA2" pad="6"/>
<connect gate="G$1" pin="REFLB1" pad="11"/>
<connect gate="G$1" pin="REFLB2" pad="12"/>
<connect gate="G$1" pin="SENSEA" pad="62"/>
<connect gate="G$1" pin="SENSEB" pad="19"/>
<connect gate="G$1" pin="SHDNA" pad="59"/>
<connect gate="G$1" pin="SHDNB" pad="22"/>
<connect gate="G$1" pin="VCMA" pad="61"/>
<connect gate="G$1" pin="VCMB" pad="20"/>
<connect gate="G$1" pin="VDD1" pad="7"/>
<connect gate="G$1" pin="VDD2" pad="10"/>
<connect gate="G$1" pin="VDD3" pad="18"/>
<connect gate="G$1" pin="VDD4" pad="63"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC2170/71/72" prefix="U">
<description>&lt;b&gt;QUAD ADC&lt;/b&gt;&lt;p&gt;
14-Bit, 125Msps/105Msps/80Msps Low Power</description>
<gates>
<gate name="G$1" symbol="LTC2173/74/75"/>
</gates>
<devices>
<device name="" package="QFN52-UKG">
<connects>
<connect gate="G$1" pin="!CS!" pad="19"/>
<connect gate="G$1" pin="AIN1+" pad="1"/>
<connect gate="G$1" pin="AIN1-" pad="2"/>
<connect gate="G$1" pin="AIN2+" pad="4"/>
<connect gate="G$1" pin="AIN2-" pad="5"/>
<connect gate="G$1" pin="AIN3+" pad="10"/>
<connect gate="G$1" pin="AIN3-" pad="11"/>
<connect gate="G$1" pin="AIN4+" pad="13"/>
<connect gate="G$1" pin="AIN4-" pad="14"/>
<connect gate="G$1" pin="DCO+" pad="36"/>
<connect gate="G$1" pin="DCO-" pad="35"/>
<connect gate="G$1" pin="ENC+" pad="17"/>
<connect gate="G$1" pin="ENC-" pad="18"/>
<connect gate="G$1" pin="FR+" pad="32"/>
<connect gate="G$1" pin="FR-" pad="31"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@45" pad="45"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="OGND" pad="33"/>
<connect gate="G$1" pin="OUT1A+" pad="44"/>
<connect gate="G$1" pin="OUT1A-" pad="43"/>
<connect gate="G$1" pin="OUT1B+" pad="42"/>
<connect gate="G$1" pin="OUT1B-" pad="41"/>
<connect gate="G$1" pin="OUT2A+" pad="40"/>
<connect gate="G$1" pin="OUT2A-" pad="39"/>
<connect gate="G$1" pin="OUT2B+" pad="38"/>
<connect gate="G$1" pin="OUT2B-" pad="37"/>
<connect gate="G$1" pin="OUT3A+" pad="30"/>
<connect gate="G$1" pin="OUT3A-" pad="29"/>
<connect gate="G$1" pin="OUT3B+" pad="28"/>
<connect gate="G$1" pin="OUT3B-" pad="27"/>
<connect gate="G$1" pin="OUT4A+" pad="26"/>
<connect gate="G$1" pin="OUT4A-" pad="25"/>
<connect gate="G$1" pin="OUT4B+" pad="24"/>
<connect gate="G$1" pin="OUT4B-" pad="23"/>
<connect gate="G$1" pin="OVDD" pad="34"/>
<connect gate="G$1" pin="PAR/!SER!" pad="47"/>
<connect gate="G$1" pin="REFH@6" pad="6"/>
<connect gate="G$1" pin="REFH@7" pad="7"/>
<connect gate="G$1" pin="REFL@8" pad="8"/>
<connect gate="G$1" pin="REFL@9" pad="9"/>
<connect gate="G$1" pin="SCK" pad="20"/>
<connect gate="G$1" pin="SDI" pad="21"/>
<connect gate="G$1" pin="SDO" pad="46"/>
<connect gate="G$1" pin="SENSE" pad="50"/>
<connect gate="G$1" pin="VCM12" pad="3"/>
<connect gate="G$1" pin="VCM34" pad="12"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@16" pad="16"/>
<connect gate="G$1" pin="VDD@51" pad="51"/>
<connect gate="G$1" pin="VDD@52" pad="52"/>
<connect gate="G$1" pin="VREF" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
