<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<library>
<packages>
<package name="BMP180">
</package>
<package name="ARDUINO_PRO_MINI_LITE">
</package>
<package name="USB3300_1">
</package>
<package name="USB3300_2">
</package>
<package name="DC-DC-STEPUP">
</package>
<package name="FTDI_UM232HB">
</package>
</packages>
<symbols>
<symbol name="BMP180">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="ARDUINO_PRO_MINI_LITE">
<pin name="2"/>
<pin name="*3"/>
<pin name="4"/>
<pin name="*5"/>
<pin name="*6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="*9"/>
<pin name="*10"/>
<pin name="*11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND"/>
<pin name="GND@2"/>
<pin name="RAW"/>
<pin name="RST"/>
<pin name="RST@2"/>
<pin name="RXI"/>
<pin name="TXO"/>
<pin name="VCC"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="USB3300">
<pin name="GND" direction="pwr"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="STP"/>
<pin name="NXT"/>
<pin name="DIR"/>
<pin name="CLK" function="clk"/>
<pin name="RST"/>
<pin name="3V3" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEPUP">
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="IN-"/>
<pin name="IN+"/>
</symbol>
<symbol name="FTDI_UM232HB">
<pin name="5V"/>
<pin name="C6"/>
<pin name="C4"/>
<pin name="C2"/>
<pin name="C0"/>
<pin name="D6"/>
<pin name="D4"/>
<pin name="D2"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D3"/>
<pin name="D5"/>
<pin name="D7"/>
<pin name="C1"/>
<pin name="C3"/>
<pin name="C5"/>
<pin name="C7"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BMP180" prefix="IC">
<gates>
<gate name="G$1" symbol="BMP180"/>
</gates>
<devices>
<device name="" package="BMP180">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_PRO_MINI_LITE">
<description>edited layout from https://github.com/sparkfun/SparkFun-Eagle-Libraries
License: https://github.com/sparkfun/SparkFun-Eagle-Libraries/blob/master/readme.md</description>
<gates>
<gate name="G$1" symbol="ARDUINO_PRO_MINI_LITE"/>
</gates>
<devices>
<device name="" package="ARDUINO_PRO_MINI_LITE">
<connects>
<connect gate="G$1" pin="*10" pad="13"/>
<connect gate="G$1" pin="*11" pad="14"/>
<connect gate="G$1" pin="*3" pad="6"/>
<connect gate="G$1" pin="*5" pad="8"/>
<connect gate="G$1" pin="*6" pad="9"/>
<connect gate="G$1" pin="*9" pad="12"/>
<connect gate="G$1" pin="12" pad="15"/>
<connect gate="G$1" pin="13" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RST@2" pad="22"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3300_?">
<gates>
<gate name="G$1" symbol="USB3300"/>
</gates>
<devices>
<device name="1" package="USB3300_1">
<connects>
<connect gate="G$1" pin="3V3" pad="19 20"/>
<connect gate="G$1" pin="5V" pad="2 4"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="5"/>
<connect gate="G$1" pin="D3" pad="7"/>
<connect gate="G$1" pin="D4" pad="9"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="DIR" pad="12"/>
<connect gate="G$1" pin="GND" pad="17 18"/>
<connect gate="G$1" pin="NXT" pad="14"/>
<connect gate="G$1" pin="RST" pad="8"/>
<connect gate="G$1" pin="STP" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="USB3300_2">
<connects>
<connect gate="G$1" pin="3V3" pad="19 20"/>
<connect gate="G$1" pin="5V" pad="1 3"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="D0" pad="2"/>
<connect gate="G$1" pin="D1" pad="4"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="10"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="14"/>
<connect gate="G$1" pin="D7" pad="16"/>
<connect gate="G$1" pin="DIR" pad="11"/>
<connect gate="G$1" pin="GND" pad="17 18"/>
<connect gate="G$1" pin="NXT" pad="13"/>
<connect gate="G$1" pin="RST" pad="7"/>
<connect gate="G$1" pin="STP" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEPUP">
<gates>
<gate name="G$1" symbol="DC-DC-STEPUP"/>
</gates>
<devices>
<device name="" package="DC-DC-STEPUP">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI_UM232HB">
<gates>
<gate name="G$1" symbol="FTDI_UM232HB"/>
</gates>
<devices>
<device name="" package="FTDI_UM232HB">
<connects>
<connect gate="G$1" pin="5V" pad="17"/>
<connect gate="G$1" pin="C0" pad="9"/>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="C3" pad="12"/>
<connect gate="G$1" pin="C4" pad="13"/>
<connect gate="G$1" pin="C5" pad="14"/>
<connect gate="G$1" pin="C6" pad="15"/>
<connect gate="G$1" pin="C7" pad="16"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="3"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="D4" pad="5"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="8"/>
<connect gate="G$1" pin="GND" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
