<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<library>
<description>&lt;b&gt;TRACO &lt;/b&gt;(R)&lt;b&gt; POWER&lt;/b&gt; DC DC Konverter&lt;p&gt;
www.tracopower.com&lt;p&gt;
Source:&lt;br&gt;
&lt;i&gt;traco.lbr&lt;/i&gt; from Bodo Fuhrmann  from Martin-Luther-Universität Halle, &amp;lt;bodo@biochemtech.uni-halle.de&amp;gt;&lt;br&gt;
&lt;i&gt;traco1.lbr&lt;/i&gt; from Hari Babu Kotte  from Mittuniversitetet,  &amp;lt;kotte_hari@rediffmail.com&amp;gt;&lt;br&gt;
Author: &lt;author&gt;librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TME-24V">
<description>&lt;b&gt;DC/DC Converter TME Series 1 Watt (24V)&lt;/b&gt;&lt;p&gt;
Source: www.tracopower.com .. tme.pdf</description>
</package>
<package name="TME">
<description>&lt;b&gt;DC/DC Converter TME Series 1 Watt (5/12V)&lt;/b&gt;&lt;p&gt;
Source: www.tracopower.com .. tme.pdf</description>
</package>
<package name="TAP2422">
<description>&lt;font color="red"&gt;&lt;b&gt;Abgekündigt&lt;/b&gt;&lt;/font&gt;</description>
</package>
<package name="TRACOPOWER2W">
<description>&lt;b&gt;DC/DC-Konverter&lt;/b&gt; 2 Watt&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tel2-d.pdf</description>
</package>
<package name="TEN3XXXX">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 3 Watt&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/ten3-d.pdf</description>
</package>
<package name="TMEXXXXS">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 1 Watt&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tme-d.pdf</description>
</package>
<package name="10515">
</package>
<package name="05105">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 5 Watt&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tpm-d.pdf</description>
</package>
<package name="TMA">
</package>
<package name="TMR-3WIE">
</package>
<package name="TSR-1">
</package>
<package name="RAC20-B">
</package>
<package name="RAC10-C">
</package>
</packages>
<symbols>
<symbol name="DC-DC-CONVERTER">
<pin name="+VIN" direction="pas"/>
<pin name="-VIN" direction="pas"/>
<pin name="+VOUT" direction="pas"/>
<pin name="-VOUT" direction="pas"/>
</symbol>
<symbol name="TAP2422">
<pin name="DC+" direction="in"/>
<pin name="DC-" direction="in"/>
<pin name="OUT+" direction="pas"/>
<pin name="0V" direction="pas"/>
<pin name="OUT-" direction="pas"/>
</symbol>
<symbol name="TRACOP1">
<pin name="+VIN" direction="in"/>
<pin name="-VIN" direction="in"/>
<pin name="+VOUT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="-VOUT" direction="pas"/>
</symbol>
<symbol name="TEN32411">
<pin name="-VIN2" direction="in"/>
<pin name="-VIN1" direction="in"/>
<pin name="+VIN2" direction="in"/>
<pin name="+VIN1" direction="in"/>
<pin name="+VOUT" direction="pas"/>
<pin name="COMMON" direction="pas"/>
</symbol>
<symbol name="TEN32423">
<pin name="-VIN2" direction="in"/>
<pin name="-VIN1" direction="in"/>
<pin name="+VIN2" direction="in"/>
<pin name="+VIN1" direction="in"/>
<pin name="+VOUT1" direction="pas"/>
<pin name="COMMON1" direction="pas"/>
<pin name="COMMON2" direction="pas"/>
<pin name="-VOUT2" direction="pas"/>
</symbol>
<symbol name="TMEXXXXS">
<pin name="E+" direction="in"/>
<pin name="E-" direction="in"/>
<pin name="A+" direction="out"/>
<pin name="A-" direction="out"/>
</symbol>
<symbol name="TPM10515">
<pin name="AC1" direction="in"/>
<pin name="AC2" direction="in"/>
<pin name="+VDC1" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="-VDC1" direction="pas"/>
<pin name="+DC2" direction="pas"/>
<pin name="-VDC2" direction="pas"/>
</symbol>
<symbol name="TPM05105">
<pin name="AC1" direction="in"/>
<pin name="AC2" direction="in"/>
<pin name="+DC" direction="pas"/>
<pin name="-DC" direction="pas"/>
</symbol>
<symbol name="TMR">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT+" direction="pas"/>
<pin name="0V" direction="pas"/>
<pin name="OUT-" direction="pas"/>
<pin name="ENA" direction="in"/>
</symbol>
<symbol name="TMR_SINGLE">
<pin name="DC+" direction="in"/>
<pin name="DC-" direction="in"/>
<pin name="OUT+" direction="pas"/>
<pin name="0V" direction="pas"/>
<pin name="ENA" direction="in"/>
</symbol>
<symbol name="TSR-1">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="RAC20-B">
<pin name="AC1"/>
<pin name="AC2"/>
<pin name="DC+"/>
<pin name="DC-"/>
</symbol>
<symbol name="RAC10-C">
<pin name="AC1"/>
<pin name="AC2"/>
<pin name="DC+"/>
<pin name="DC-"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TME?*" prefix="V">
<description>&lt;b&gt;DC/DC Converter TME Series 1 Watt &lt;/b&gt;&lt;p&gt;
Source: www.tracopower.com .. tme.pdf</description>
<gates>
<gate name="G$1" symbol="DC-DC-CONVERTER"/>
</gates>
<devices>
<device name="05" package="TME">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="05S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0505S"/>
<attribute name="OC_FARNELL" value="1007538"/>
<attribute name="OC_NEWARK" value="51R5321"/>
</technology>
<technology name="09S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0509S"/>
<attribute name="OC_FARNELL" value="1007539"/>
<attribute name="OC_NEWARK" value="51R5322"/>
</technology>
<technology name="12S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0512S"/>
<attribute name="OC_FARNELL" value="1007540"/>
<attribute name="OC_NEWARK" value="51R5323"/>
</technology>
<technology name="15S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0515S"/>
<attribute name="OC_FARNELL" value="1007541"/>
<attribute name="OC_NEWARK" value="51R5324"/>
</technology>
</technologies>
</device>
<device name="24" package="TME-24V">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="05S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2405S"/>
<attribute name="OC_FARNELL" value="1007547"/>
<attribute name="OC_NEWARK" value="51R5329"/>
</technology>
<technology name="09S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2409S"/>
<attribute name="OC_FARNELL" value="1007548"/>
<attribute name="OC_NEWARK" value="51R5330"/>
</technology>
<technology name="12S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2412S"/>
<attribute name="OC_FARNELL" value="1007549"/>
<attribute name="OC_NEWARK" value="51R5331"/>
</technology>
<technology name="15S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2415S"/>
<attribute name="OC_FARNELL" value="1007550"/>
<attribute name="OC_NEWARK" value="51R5332"/>
</technology>
</technologies>
</device>
<device name="12" package="TME">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="3"/>
</connects>
<technologies>
<technology name="05S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1205S"/>
<attribute name="OC_FARNELL" value="1007542"/>
<attribute name="OC_NEWARK" value="51R5325"/>
</technology>
<technology name="09S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1209S"/>
<attribute name="OC_FARNELL" value="1007544"/>
<attribute name="OC_NEWARK" value="51R5326"/>
</technology>
<technology name="12S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1212S"/>
<attribute name="OC_FARNELL" value="1007545"/>
<attribute name="OC_NEWARK" value="51R5327"/>
</technology>
<technology name="15S">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1215S"/>
<attribute name="OC_FARNELL" value="1007546"/>
<attribute name="OC_NEWARK" value="51R5328"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAP2422" prefix="PWS" uservalue="yes">
<description>&lt;font color="red"&gt;&lt;b&gt;Abgekündigt&lt;/b&gt;&lt;/font&gt; Ersetzt durch TEN 15 Serie,</description>
<gates>
<gate name="G$1" symbol="TAP2422"/>
</gates>
<devices>
<device name="" package="TAP2422">
<connects>
<connect gate="G$1" pin="0V" pad="COM"/>
<connect gate="G$1" pin="DC+" pad="+VIN"/>
<connect gate="G$1" pin="DC-" pad="-VIN"/>
<connect gate="G$1" pin="OUT+" pad="+VOUT"/>
<connect gate="G$1" pin="OUT-" pad="-VOUT"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEL_2-" prefix="PWS">
<description>&lt;b&gt;DC/DC-Konverter&lt;/b&gt; 2 Watt, 1 x Input, 1 x +- Output&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tel2-d.pdf</description>
<gates>
<gate name="G$1" symbol="TRACOP1"/>
</gates>
<devices>
<device name="" package="TRACOPOWER2W">
<connects>
<connect gate="G$1" pin="+VIN" pad="16"/>
<connect gate="G$1" pin="+VOUT" pad="9"/>
<connect gate="G$1" pin="-VIN" pad="1"/>
<connect gate="G$1" pin="-VOUT" pad="10"/>
<connect gate="G$1" pin="COM" pad="8"/>
</connects>
<technologies>
<technology name="0521">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-0521"/>
<attribute name="OC_FARNELL" value="1007027"/>
<attribute name="OC_NEWARK" value="51R4755"/>
</technology>
<technology name="0522">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-0522"/>
<attribute name="OC_FARNELL" value="1007028"/>
<attribute name="OC_NEWARK" value="51R4756"/>
</technology>
<technology name="0523">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-0523"/>
<attribute name="OC_FARNELL" value="1007029"/>
<attribute name="OC_NEWARK" value="51R4757"/>
</technology>
<technology name="1221">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-1221"/>
<attribute name="OC_FARNELL" value="1007032"/>
<attribute name="OC_NEWARK" value="51R4760"/>
</technology>
<technology name="1222">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-1222"/>
<attribute name="OC_FARNELL" value="1007033"/>
<attribute name="OC_NEWARK" value="51R4761"/>
</technology>
<technology name="1223">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-1223"/>
<attribute name="OC_FARNELL" value="1007034"/>
<attribute name="OC_NEWARK" value="51R4762"/>
</technology>
<technology name="2421">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-2421"/>
<attribute name="OC_FARNELL" value="1007039"/>
<attribute name="OC_NEWARK" value="51R4765"/>
</technology>
<technology name="2422">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-2422"/>
<attribute name="OC_FARNELL" value="1007041"/>
<attribute name="OC_NEWARK" value="51R4766"/>
</technology>
<technology name="2423">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-2423"/>
<attribute name="OC_FARNELL" value="1007042"/>
<attribute name="OC_NEWARK" value="51R4767"/>
</technology>
<technology name="4821">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-4821"/>
<attribute name="OC_FARNELL" value="1007045"/>
<attribute name="OC_NEWARK" value="51R4770"/>
</technology>
<technology name="4822">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-4822"/>
<attribute name="OC_FARNELL" value="1007046"/>
<attribute name="OC_NEWARK" value="51R4771"/>
</technology>
<technology name="4823">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEL 2-4823"/>
<attribute name="OC_FARNELL" value="1007047"/>
<attribute name="OC_NEWARK" value="51R4772"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEN_3*" prefix="PWS">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 3 Watt, 2 x Input, 1 x Output&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/ten3-d.pdf</description>
<gates>
<gate name="G$1" symbol="TEN32411"/>
</gates>
<devices>
<device name="" package="TEN3XXXX">
<connects>
<connect gate="G$1" pin="+VIN1" pad="22"/>
<connect gate="G$1" pin="+VIN2" pad="23"/>
<connect gate="G$1" pin="+VOUT" pad="14"/>
<connect gate="G$1" pin="-VIN1" pad="2"/>
<connect gate="G$1" pin="-VIN2" pad="3"/>
<connect gate="G$1" pin="COMMON" pad="16"/>
</connects>
<technologies>
<technology name="0510">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0511">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0513">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1210">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1211">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1212">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1213">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2410">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2411">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN3-2411"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="45K1582"/>
</technology>
<technology name="2412">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2413">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN3-2413"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14N5516"/>
</technology>
<technology name="4810">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4811">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN 3-4811WI"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90R9814"/>
</technology>
<technology name="4812">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4813">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEN_3--*" prefix="PWS">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 3 Watt, 2 x Input, 2 x Output&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/ten3-d.pdf</description>
<gates>
<gate name="G$1" symbol="TEN32423"/>
</gates>
<devices>
<device name="" package="TEN3XXXX">
<connects>
<connect gate="G$1" pin="+VIN1" pad="22"/>
<connect gate="G$1" pin="+VIN2" pad="23"/>
<connect gate="G$1" pin="+VOUT1" pad="14"/>
<connect gate="G$1" pin="-VIN1" pad="2"/>
<connect gate="G$1" pin="-VIN2" pad="3"/>
<connect gate="G$1" pin="-VOUT2" pad="11"/>
<connect gate="G$1" pin="COMMON1" pad="9"/>
<connect gate="G$1" pin="COMMON2" pad="16"/>
</connects>
<technologies>
<technology name="0521">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0522">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN 3-0522"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="91R2128"/>
</technology>
<technology name="0523">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="122">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1221">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN31221"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="60R5780"/>
</technology>
<technology name="1223">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2421">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2422">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN 3-2422WI"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="78R5872"/>
</technology>
<technology name="2423">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TEN3-2423"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="72J5373"/>
</technology>
<technology name="4821">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4822">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4823">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TME_*S" prefix="PWS">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 1 Watt&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tme-d.pdf</description>
<gates>
<gate name="G$1" symbol="TMEXXXXS"/>
</gates>
<devices>
<device name="" package="TMEXXXXS">
<connects>
<connect gate="G$1" pin="A+" pad="4"/>
<connect gate="G$1" pin="A-" pad="3"/>
<connect gate="G$1" pin="E+" pad="2"/>
<connect gate="G$1" pin="E-" pad="1"/>
</connects>
<technologies>
<technology name="0505">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0505S"/>
<attribute name="OC_FARNELL" value="1007538"/>
<attribute name="OC_NEWARK" value="51R5321"/>
</technology>
<technology name="0509">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0509S"/>
<attribute name="OC_FARNELL" value="1007539"/>
<attribute name="OC_NEWARK" value="51R5322"/>
</technology>
<technology name="0512">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0512S"/>
<attribute name="OC_FARNELL" value="1007540"/>
<attribute name="OC_NEWARK" value="51R5323"/>
</technology>
<technology name="0515">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 0515S"/>
<attribute name="OC_FARNELL" value="1007541"/>
<attribute name="OC_NEWARK" value="51R5324"/>
</technology>
<technology name="1205">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1205S"/>
<attribute name="OC_FARNELL" value="1007542"/>
<attribute name="OC_NEWARK" value="51R5325"/>
</technology>
<technology name="1209">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1209S"/>
<attribute name="OC_FARNELL" value="1007544"/>
<attribute name="OC_NEWARK" value="51R5326"/>
</technology>
<technology name="1212">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1212S"/>
<attribute name="OC_FARNELL" value="1007545"/>
<attribute name="OC_NEWARK" value="51R5327"/>
</technology>
<technology name="1215">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 1215S"/>
<attribute name="OC_FARNELL" value="1007546"/>
<attribute name="OC_NEWARK" value="51R5328"/>
</technology>
<technology name="2405">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2405S"/>
<attribute name="OC_FARNELL" value="1007547"/>
<attribute name="OC_NEWARK" value="51R5329"/>
</technology>
<technology name="2409">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2409S"/>
<attribute name="OC_FARNELL" value="1007548"/>
<attribute name="OC_NEWARK" value="51R5330"/>
</technology>
<technology name="2412">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2412S"/>
<attribute name="OC_FARNELL" value="1007549"/>
<attribute name="OC_NEWARK" value="51R5331"/>
</technology>
<technology name="2415">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TME 2415S"/>
<attribute name="OC_FARNELL" value="1007550"/>
<attribute name="OC_NEWARK" value="51R5332"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPM-*" prefix="PWS" uservalue="yes">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 10/15 Watt, 1 x Input, 2 x Output&lt;p&gt;
Suurce: http://www.tracopower.com/datasheet_g/tpm-d.pdf</description>
<gates>
<gate name="G$1" symbol="TPM10515"/>
</gates>
<devices>
<device name="" package="10515">
<connects>
<connect gate="G$1" pin="+DC2" pad="4"/>
<connect gate="G$1" pin="+VDC1" pad="3"/>
<connect gate="G$1" pin="-VDC1" pad="7"/>
<connect gate="G$1" pin="-VDC2" pad="6"/>
<connect gate="G$1" pin="AC1" pad="1"/>
<connect gate="G$1" pin="AC2" pad="2"/>
<connect gate="G$1" pin="COM1" pad="5"/>
</connects>
<technologies>
<technology name="05212">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="05215">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPM_*" prefix="PWS">
<description>&lt;b&gt;DC/DC Konverter&lt;/b&gt; 5 Watt, 1 x Input, 1 x Output&lt;p&gt;
Source: http://www.tracopower.com/datasheet_g/tpm-d.pdf</description>
<gates>
<gate name="G$1" symbol="TPM05105"/>
</gates>
<devices>
<device name="" package="05105">
<connects>
<connect gate="G$1" pin="+DC" pad="3"/>
<connect gate="G$1" pin="-DC" pad="4"/>
<connect gate="G$1" pin="AC1" pad="1"/>
<connect gate="G$1" pin="AC2" pad="2"/>
</connects>
<technologies>
<technology name="05105">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="05112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMA_*" prefix="DC">
<description>&lt;p&gt; DC/DC-Konverter TMA Serie 1 Watt &lt;/p&gt;
&lt;br&gt;
&lt;br&gt;
Die TMA-Serie sind ultrakleine, isolierte 1 W DC/DC-Konverter im
SIL-Gehäuse. Mit dem kleinen Platzbedarf von nur 1.2 cm2 sind sie
die ideale Lösung zur Spannungsumsetzung oder -isolierung auf
Printkartenebene. Dank SMD-Technologie sind diese Wandler sehr
zuverlässig und kostengünstig.
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="TAP2422"/>
</gates>
<devices>
<device name="DUAL" package="TMA">
<connects>
<connect gate="G$1" pin="0V" pad="5"/>
<connect gate="G$1" pin="DC+" pad="1"/>
<connect gate="G$1" pin="DC-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="6"/>
<connect gate="G$1" pin="OUT-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SINGLE" package="TMA">
<connects>
<connect gate="G$1" pin="DC+" pad="1"/>
<connect gate="G$1" pin="DC-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="6"/>
<connect gate="G$1" pin="OUT-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMR-3WIE" prefix="TR">
<description>&lt;p&gt;Traco Power - TMR 3WIE Series, 3 Watt&lt;/p&gt;

&lt;br&gt;&lt;br&gt;
Features:&lt;br&gt;
? Wide 4:1 input voltage range&lt;br&gt;
? Compact SIP-8 package&lt;br&gt;
? Cost optimized design&lt;br&gt;
? Temperature range ?40°C to +85°C&lt;br&gt;
? I/O isolation 1600 VDC&lt;br&gt;
? Remote On/Off control&lt;br&gt;
? 3-year product warranty&lt;br&gt;
&lt;br&gt;
4811 - 5V Single&lt;br&gt;
4822 - +/-12V Dual
&lt;br&gt;&lt;br&gt;
http://docs-europe.electrocomponents.com/webdocs/1176/0900766b81176cfe.pdf</description>
<gates>
<gate name="TR" symbol="TMR"/>
</gates>
<devices>
<device name="TMR-3-4822WIE" package="TMR-3WIE">
<connects>
<connect gate="TR" pin="0V" pad="7"/>
<connect gate="TR" pin="ENA" pad="3"/>
<connect gate="TR" pin="IN+" pad="2"/>
<connect gate="TR" pin="IN-" pad="1"/>
<connect gate="TR" pin="OUT+" pad="6"/>
<connect gate="TR" pin="OUT-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMR-3WIE_SINGLE" prefix="TR">
<gates>
<gate name="TR" symbol="TMR_SINGLE"/>
</gates>
<devices>
<device name="" package="TMR-3WIE">
<connects>
<connect gate="TR" pin="0V" pad="7"/>
<connect gate="TR" pin="DC+" pad="2"/>
<connect gate="TR" pin="DC-" pad="1"/>
<connect gate="TR" pin="ENA" pad="3"/>
<connect gate="TR" pin="OUT+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSR-1" prefix="IC">
<description>&lt;p&gt;DC/DC Converters - TSR-1 Series, 1 A &lt;/p&gt;&lt;br&gt;

&lt;b&gt;Features:&lt;/b&gt;&lt;br&gt;
◆ Up to 96 % efficiency – No heat-sink required&lt;br&gt;
◆ Pin compatible with LMxx linear regulators&lt;br&gt;
◆ SIP-package fits existing TO-220 footprint&lt;br&gt;
◆ Built in filter capacitors&lt;br&gt;
◆ Operation temp. range –40°C to +85°C&lt;br&gt;
◆ Short circuit protection&lt;br&gt;
◆ Wide input operating range&lt;br&gt;
◆ Excellent line / load regulation&lt;br&gt;
◆ Low standby current&lt;br&gt;
◆ 3-year product warranty&lt;br&gt;
&lt;br&gt;
The new TSR-1 series step-down switching regulators are drop-in replacement for
inefficient 78xx linear regulators. A high efficiency up to 96 % allows full load
operation up to +60°C ambient temperature without the need of any heat-sink or
forced cooling.&lt;br&gt;
The TSR-1 switching regulators provide other significant features over linear regulators,
i.e. better output accuracy (±2 %), lower standby current of 2 mA and no
requirement of external capacitors. The high efficiency and low standby power
consumption makes these regulators an ideal solution for many battery powered
applications.
&lt;br&gt; &lt;b&gt;
For input voltage higher than 32 VDC an input capcitor 22uF / 50 V is required. &lt;/b&gt;</description>
<gates>
<gate name="IC" symbol="TSR-1"/>
</gates>
<devices>
<device name="" package="TSR-1">
<connects>
<connect gate="IC" pin="GND" pad="2"/>
<connect gate="IC" pin="IN" pad="1"/>
<connect gate="IC" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RAC10" prefix="PS">
<description>&lt;p&gt;10 Watt Single AC/DC-Converter &lt;/p&gt;&lt;br&gt;
&lt;b&gt;Features&lt;/b&gt;&lt;br&gt;
● Very Compact Low AC/DC Power Supply&lt;br&gt;
● High Efficiency&lt;br&gt;
● Single &amp; Dual Output Options&lt;br&gt;
● Continuous Short Circuit Protection&lt;br&gt;
● Isolated Output 3.75kVAC/1 min&lt;br&gt;
● EN55022 Class B Compliant&lt;br&gt;
● High Operating Temperature&lt;br&gt;
● Low Standby Power Consumption&lt;br&gt;</description>
<gates>
<gate name="PS" symbol="RAC10-C"/>
</gates>
<devices>
<device name="" package="RAC10-C">
<connects>
<connect gate="PS" pin="AC1" pad="1"/>
<connect gate="PS" pin="AC2" pad="2"/>
<connect gate="PS" pin="DC+" pad="4"/>
<connect gate="PS" pin="DC-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMR3-1223" prefix="TR">
<description>&lt;p&gt;Traco Power - TMR 3WIE Series, 3 Watt&lt;/p&gt;

&lt;br&gt;&lt;br&gt;
Features:&lt;br&gt;
? Wide 4:1 input voltage range&lt;br&gt;
? Compact SIP-8 package&lt;br&gt;
? Cost optimized design&lt;br&gt;
? Temperature range ?40°C to +85°C&lt;br&gt;
? I/O isolation 1600 VDC&lt;br&gt;
? Remote On/Off control&lt;br&gt;
? 3-year product warranty&lt;br&gt;
&lt;br&gt;
4811 - 5V Single&lt;br&gt;
4822 - +/-12V Dual
&lt;br&gt;&lt;br&gt;
http://docs-europe.electrocomponents.com/webdocs/1176/0900766b81176cfe.pdf</description>
<gates>
<gate name="TR" symbol="TMR"/>
</gates>
<devices>
<device name="TMR3-1223" package="TMR-3WIE">
<connects>
<connect gate="TR" pin="0V" pad="7"/>
<connect gate="TR" pin="ENA" pad="3"/>
<connect gate="TR" pin="IN+" pad="2"/>
<connect gate="TR" pin="IN-" pad="1"/>
<connect gate="TR" pin="OUT+" pad="6"/>
<connect gate="TR" pin="OUT-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
